This version is to accommodate the customer (Bluefin etc) and the IOPW downlink is set to 80 Mb LVDS link. Top level was modified to accommodate this rather than write a whole new module to have a RS232/80Mb uplink methodology.

Rev Register 8022
20 MHz beam former bus speed

Single uplink (dual uplink seems to cause excessive heating)
AUV system
IOPW has 80 Mb downlink

DSP read interface deactivated since the PHY is not used (minimize logic to get timing requirement with greater ease)

PLK10, PLK9 are sequenced on in approximately 50 ms intervals (does not seem to reset)

PLK7, PLK6 are not switched on

This code will be released to the firmware downloader
