(footprint "DELEVAN_CM6460-335"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "DELEVAN_CM6460-335"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.08 -5.08)
		(size 3.048 3.048)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "2" smd rect
		(at -5.08 5.08)
		(size 3.048 3.048)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "3" smd rect
		(at 5.08 5.08)
		(size 3.048 3.048)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "4" smd rect
		(at 5.08 -5.08)
		(size 3.048 3.048)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
)
