It’s a bit confusing, but the lines I was told to do were in green.
1.	Some kind of external hardening of the power module
2.	Replacing the camera (not the lens) due to EOL
3.	Manipulator head
4.	OCS CPU change due to EOL
5.	Adding the strain relief block
6.	Adding the DAGR cable
7.	Thruster refill attachment
