
PARAGRAPH of CZE-93-105A (Paragraph of CZE-93A-105A SAASM)
PARAGRAPH TITLE
ALLOCATION
VERIFICATION
COMMENTS


5.4
Physical Security Verification
A
I
See log/slide attached


5.4.1
All PPS HAE end items marked.
A
I
Drawing attached (See 2.2)


5.4.2
Fill port directly routes keys
A
I
Fill port directly to MPE-S


5.4.3
Data port route keys…
A
I
Not implemented (Pins 37 to 41 for Radio fill device of MPE-S are not used on wiring diagram Y216E349)


5.4.4
Connections between …
NA

Not applicable to SAASM


5.4.5
No GPS security…
A
I
Satisfied by Rockwell Collins MPE-S


5.5
Functional Security Verification
A
I
See Log/slide attached


5.5.1
Keys are loaded via fill or data port.
A
I
Loading keys through CYZ-10 (Wiring diagram Y216E349), data port not implemented


5.5.2
Keys and temporary key storage.
A
D
1) Zeroization tested 1 and discrete J1-1), Zeroization with Verification 

2) Temporary keys not implemented.


5.5.3
After a total loss of power keys are automatically zeroized…
A
D
MPE-S complies


5.5.4
Keys are zeroized with auxiliary power
NA

No cold Zeroization


5.5.5
Functionality of SA…
NA

Satisfied by Rockwell Collins MPE-S


5.5.6
Other Security related…
NR

Nothing required by JPO


5.6
GPS JPO Contact
NR

Information only

