Precision Underwater Positioning for in-situ Laser Raman Spectrographic Applications
The Monterey Bay Aquarium Research Institute (MBARI) has developed and deployed a Laser Raman Spectrometer (LRS) for in-situ measurements in the deep ocean. Quality spectra have been obtained of standards carried to the seafloor. The next stage of this development

involves the ability to obtain spectra from natural targets of interest in the deep ocean and to maximize signal return from the sample. To accomplish maximum signal return the LRS probe head must be properly positioned with respect to the sample. This is in contrast to laboratory work in which the sample is precisely positioned with respect to the probe head.This requirement has been the driver for a new device, the Precision Underwater Positioning system (PUP).

The positioning system has strict requirements for motion about the target. The LRS requires very exact and repeatable motions with positional accuracies in the 1 mm range over a large workspace. The device must also let the user see where they are focusing, be able to 

move without disturbing the base position, and to stay stable over a variety of terrains. The system must also adapt to two separate power systems. The PUP system also has the requirement of returning relative position from a known home position once set in place. The device also has several operational constraints that impacted the design and operation of the system.

This paper outlines the science drivers, the operational considerations, and the engineering trades that were made to build the first two stages of the PUP. The test results of this system are also included demonstrating the devices actual performance against the 

specifications. In conclusion the paper outlines the next tasks and the direction the program is taking to fulfill the complete precision underwater positioning system requirements.
