See Actuator Notes, pp. 14-15

Rudder Angle Linear Actuator Displacement Command, Counts

Out1 sin(u[1])*rR1 + cos(u[1])*rR2

k2 cos(u[1])*rR1 - sin(u[1])*rR2

k1 sqrt( (u[1]-xRR)^2 + (u[2]-aR)^2 )

dist signal1

signal2 m2c Gain3

disp0

Actuator Length, Center Position

In1 2 <deltaRCmd>

Rudder Counts

Actu Length

/u/rob/altex/sim/AltexSim2.mdl

AltexSim2/Tailcone Micro/Rudder Angle to Counts

page 12/16 printed 05-Oct-1999 17:02