This generates one cycle of cross-current bewteen the start and waypoint WP1.

Out2

1

Out1

r_No_WP1_N_x Wavelength

Terminator

Selector

Product1 r_No_Bo_N_x signal2 sin(2*pi*u[1]/u[2])

Fcn vel_C_N_N_y Disturbance Current, Coord in EF1 vel_C_N_N_x Disturbance Current, Coord in EF

In1 24 r_No_Bo_N_x 2 v_C_N_N_y v_C_N_N_x

/u/rob/altex/sim/AltexSim2.mdl

AltexSim2/Vehicle/Ocean Current Model

page 14/16 printed 05-Oct-1999 17:02