.2 rad/sec is the Odyssey max. slew rate

1

Out1

[p] tag1

[theta] tag

[p] r1

Zero-Order Hold3

Zero-Order Hold2

Zero-Order Hold1

Zero-Order Hold

Terminator2

Sum2

Sum1 Sum

In1 Out1

Shortest Slew

Selector

Saturation

-1 SNAME Def

Max Rate Kpp Kph

Kip Kip

Kdp Kdp KdppIx

Goto2

KppErrorIx Goto

[theta] From1

Tz z-1 Discrete-Time Integrator

Demux In2

In1

r deltaECmd

<pitchCmd>

2 24

Heading

Psi

/u/rob/altex/sim/AltexSim2.mdl

AltexSim2/Dynamic Control/Pitch Control

page 6/16 printed 05-Oct-1999 17:02