	System
	Accuracy
	Cost
	Power
	Constraint

	GPS
	150-1m
	< 1K
	O(1 W)
	Surface only

	Doppler Velocity Log
	~1% Dist. Travel
	25 K
	25 W
	1m-500m Altitude

	Correlation Velocity Log
	~1% Dist Travel
	?
	?
	>500m

	Long Baseline Acoustic Navigation
	5 cm @ 100 m

3 m @ 10 km
	> 100 K
	O(5 W)
	Calibration and deployment

	USBL Acoustic Navigation
	.1% to 10% of Slant Range
	>100k
	0(30 W)
	Telemetry from Surface

	Inertial Navigation System
	1 nm/hr (unaided)
	80 K
	35 W
	Initialization

	INS/DVL
	.05 to .1% Dist Travel
	150 K
	45-60 W
	Initialization


