Mission Summary

Note: Missions that were very short, or otherwise inconsequential,  are omitted.

1. 8 October - A fjord near Tromso, where we almost lost the vehicle.  700 1.66’ N, 200 17.196’ E.  The vehicle had a single midbody with the Kearfott DVL pointing down.

8 October:   Short Vehicle, Kft up, 70 01.66', 20 17.196'.  Fjord near Tromso  where we almost lost it.

	Name
	281.03

	UTC Time
	12:26

	Duration, Min.
	5 

	Depth, meters
	15

	Description
	Straight and level setpoint at heading 050

	Comments
	· Ran the wrong mission.

· The vehicle appeared to be very heavy in the bow, and could not achieve level flight.  It terminated on the depth envelope at 35 meters.

· There is an abrupt, albeit temporary, pitch up.  It looks like the vehicle hit something.  

· The vehicle was detected on the surface but was not found visually for several hours.


10 October:  Short Vehicle, Kerfott up, 79 8.17', 31 59.2897'.

	Name
	283.00

	UTC Time
	12:36

	Duration, Min.
	4

	Depth, meters
	15

	Description
	Straight and level setpoint at heading 300T

	Comments
	· Ran to competion.

· Comms failed soon after the mission

· Data not in the repository.


13 October: Short Vehicle, Kft up, 81 50.335', 21 50.367'.  No ice in sight.

	Name
	286.00

	UTC Time
	06:59

	Duration, Min.
	4

	Depth, meters
	15

	Description
	Straight and level setpoint at heading 130T

	Comments
	· Ran to competion.

· Depth performance was poor because the Nav algorithm was still interpreting range from the now-upward looking DVL as altitude.

· Inertial Nav Data corrupted by the DVL.


	Name
	286.01

	UTC Time
	07:21

	Duration 
	550 seconds

	Depth, meters
	15

	Description
	Straight and level setpoint at heading 240T

	Comments
	· Set the minimum altitude small to avoid the above problem

· Ran to competion.

· Steady-state heading error of +/- .5 degrees.  Rudder trimmed 2.3 degrees to starboard.

· Depth control not steady-state, but looks good

· Inertial Nav Data corrupted by the DVL.

· Science sensors working.  The IPS depth shows an initial offset from the parosci, but this error decreases over time.  The parosci appeared to be in error by 4.2 meters when the vehicle surfaced.


	Name
	286.02

	UTC Time
	07:45

	Duration, Min.
	15

	Depth, meters
	25

	Description
	Out & back; 600 sec. at 290T, then 200 sec at 110.

	Comments
	· Ran to competion.

· Depth control +/- 1 meter.  Elevator trimmed -4.7 degrees.

· Parosci had accrued a 4 meter error by the end

· Heading control error +/- .5 degrees. 

· Inertial Nav Data corrupted by the DVL.

· Science data looks OK


	Name
	286.03

	UTC Time
	08:26

	Duration, Min.
	15

	Depth, meters
	20

	Description
	Straight at 180T for 400 sec, then back at 340T, 300 sec.  Yoyo on both legs.

	Comments
	· Yoyos failed due to incorrect min depth setting.

· Mission ran to completion, but was running on the surface for several minutes.

· Inertial Nav Data corrupted by the DVL.


	Name
	286.04

	UTC Time
	08:53

	Duration, Min.
	25

	Depth, meters
	25

	Description
	Straight and level setpoint at heading 90T for 7 min, then 270 for 14 min.

	Comments
	· Ran to competion.

· Steady-state depth control error +/- 60 cm.

· Elevator trimmed to -5.3 degrees.

· Steady-state heading error +/- .7 degrees.

· Rudder trimmed to -1.4 degrees

·  Steady-state roll angle 2 degrees.

· Inertial Nav Data corrupted by the DVL.

· Science data looks good.


	Name
	286.06

	UTC Time
	09:32

	Duration, Min.
	5

	Depth, meters
	25

	Description
	Straight and level setpoint at heading 200T for 4 minutes.

	Comments
	· Ran to competion.

· DVL input to the Kearfott disabled.  Inertially determined position is continuous.

· Dive rate 9 meters/min under pitch control set at -10 degrees.

· The mission was too short to measure steady-state errors.

· DVL appeared to briefly achieve bottom lock


	Name
	286.07

	UTC Time
	09:45

	Duration, Min.
	12

	Depth, meters
	25

	Description
	Straight and level setpoint at heading 300T for 700 seconds

	Comments
	· Ran to competion.

· DVL input to the Kearfott disabled.  Inertially determined position is continuous.

· Unexplained pitch excursion at 480 seconds.  Water currents?

· 4 meter parsoci error again at the end.

· The mission was too short to measure steady-state errors.

· Science data is interesting.  There is a large temperature change at 25 meters.


	Name
	286.08

	UTC Time
	10:03

	Duration, Min.
	8

	Depth, meters
	15

	Description
	Straight and level setpoint at heading 160T for 700 seconds. Test acoustic abort.

	Comments
	· Ran until aborted.

· DVL input to the Kearfott disabled.  Inertially determined position is continuous.

· Large depth transient probably due to the descend behavior’s termination depth being set the same as the depth setpoint.

· The mission was too short to measure steady-state errors.


16 October: Short Vehicle, Kft up, 82 36.72', 11 13.56'.

	Name
	289.01

	UTC Time
	11:55

	Duration, Min.
	15

	Depth, meters
	50

	Description
	Straight and level setpoint at heading 120T for 120 sec., then 300T for 100 sec.  Then pitch control +10 degrees.  Spiral ascent with a pitch setpoint of +15 degrees.

	Comments
	· Ran to completion

· DVL input to the Kearfott disabled.  Inertially determined position is continuous.

· Ascent rate of 25 meters/min during pitch setpoint of +10 deg
· Vehicle appeared to have reached the surface earlier than anticipated, and ended up circling on the surface during the (planned) ascent.
· Dvl axes still incorrect.  The Dvl appeared to track something, perhaps a piece of ice.  Water track disabled.

· The mission was too short to measure steady-state errors.

· CTD working, but flow to #2 appears partially blocked by ice crystals.

· Isus in test mode.

· Ips4 shut off.


	Name
	289.03

	UTC Time
	12:34

	Duration, Min.
	45

	Depth, meters
	30

	Description
	First long under-ice run.  170T for 15 min, then 350.

	Comments
	· Ran until aborted in the lead, as planned.
· Inertal nav again corrupted by bad Dvl readings.
· Depth control +/- 1 meter, but appears to be slowly damping out with a period of 210 seconds.  This mode is excited again at the turn, and again damps out.
· Commanded pitch +/- 2 degrees with the 210 sec period.  Pitch control error is +/- 1.5 degrees, but with a period of 10 seconds.


289.03 - FIRST long under ice run.  50m depth, 30 Min.  Ips and Isus were 

         shut OFF.

** Short Vehicle, Kft up, 82 34.86', 11 54.14', 17 Oct.

290.04 - Wouldn't dive ???

290.06 - 8 min. run.  Ips log empty.

290.08 - 30 Min. under ice run.  Spiral down to 50 m, 350 for 15 min, 170

         for 15 min, spiral up.  

**  Long Vehicle, 81 57', 12 10'E **

291.00-04 - Not recorded.  These were probably runs on deck.

291.05 - Failed to run due to Ips abort.

291.06 - Aborted by the operator because of failure to dive. 

           - The descent behavior was using pitch control with a 10 Degree 

             setpoint.

291.07 - Aborted by the operator because it failed to dive and

         a collision with the ice was imminent.

           - Pitch control; 10 Degrees.

291.08 - Aborted by the operator because of failure to dive. 

           - Pitch control; 15 Degrees.

291.09 - Aborted by the operator because of failure to dive. 

           - Pitch control; 5 Degrees.

291.10 - Aborted by the operator because of failure to dive. 

           - 10 Sec surface run followed by 15 Sec of  Deg pitch up.


   - No ips log.

291.11 - Aborted by the operator because the vehicle was in a patch of ice.

291.12 - The small boat assisted this launch.

           - Vehicle dove.


   - The operator issued an acoustic abort, but the vehicle had


     aborted moments early due to an IPS driver crash.


   - Comms were lost.


   - 25 Meters, 3 Min.

On Deck:   - Drew & crew reballasted the vehicle.

           - Sib & Hans fixed the comms problem.


   - Parosci problem ocurred.  Drew & crew fixed it.

Software Changes:  

 - Added code to prevent non-essential sensor from aborting the mission.

 - Hans?

** Long Vehicle, 81 40.5',  12 42.7' Kft up **

292.00-05 - Deck runs.

292.06 - Octans driver crash aborted the mission moments after it started.


   - Operator removed octansServer from devices.cfg.


   - Crossbow now provides heading.

292.07 - Aborted by the operator because of failure to dive. 

           - Lost comms?

292.08 - The vehicle dove but the depth envelope terminated the mission

         because of a depth overrun.

           - Vehicle was 78 Deg bow down.


   - Long inital surface run.


   - Launch had -10 Degree pitch control.


   - 15 Meters, 5 Min.


   - Ips aborted at 225 sec.


   - CTD interesting.

292.09 - Out & back.  The vehicle dove and the mission was not prematurely terminated.

           - 20 Meters


   - No flow measurement on CTD2


   - Depth/Pitch control marginal.


   - There are some Parosci dropouts.


   - Dvl water layer tracking good.


   - Kearfott position estimate reasonable.

292.10 - 7 Minute out & back.  Mission ran to completion.

           - Depth/Pitch control marginal.


   - Ips died at 225 Seconds.


   - Dvl water layer tracking giving reasonable results.


   - Kearfott position estimate reasonable.


   - There are some Parosci dropouts.


   - Battery low.

** Long Vehicle; Kft up; 80 44.298'; 16 35.068' **

296.09 - First attempted buoy launch. Straight, then circle for 15


 min, at 50 meters.

296.10 - Unreachable waypoint test; 10 min, 30 meters

296.11 - Unreachable waypoint test; 14 min, 25 meters

** Open water deep sections near Svalbard, Short Vehicle, no Ips, Kft Down **

   81 00.756'; 16 07.354'

297.03 - Yoyo to 500 m.  Partial waypoint followed by a setpoint.  

          - The headings were supposed to be identical, but are obviously

            different in the Nav Plot.  Possible causes are cross current or

            initial position error.

          - Dvl water lock poor.  Lock vs. lost appears periodic, perhaps due

            to water mass and bottom pings interleaved.

          - Good CTD data.

          - Speed variation due caused by climb/descend is 1.5/1.1 m/sec.

          - Propulsion was using 1.5 Amps more to descend.

297.04 - Yoyo to 500 m with setpoint only.  

          - Rudder trimmed 2 degrees to starboard. 

          - Science data.

297.05 - Yoyo to 500 m

          - Octans hosed.

          - Science data.

** Under Ice Triangle Runs, Short Vehicle with Ips, Kft Down **

   81 15.0340; 15 34.8450'  

298.00 - 1350 meter triangle partially under ice, Ips active, 30 meters

          - Depth/Pitch control poor;  1 meter for the first leg, but

            it subsequently decreases to half that.  External disturbance

            or transient?

          - Spiral ascent and descent

          - Kearfott nav hosed.

          - Dvl water lock extremely poor.

          - Parosci noisy.

          - Science data looks good.

          - Elevator trimmed to -1 Deg.

298.03 - 1350 meter triangle partially under ice, Ips active, 30 meters

          - Elevator trimmed to -4 Deg; nose heavy or too buoyant??

298.05 - 1350 meter triangle partially under ice, Ips active, 30 meters

          - Depth/Pitch control not smooth;  approx. 60 cm in depth. ?


  - Setpoint control


  - Rudder and Elevator appear to have a 2 degree deadband


  - Dvl water lock never achieved

          - Dvl temperature measurement now looks whacky

298.06 - 500m North, 2500m @ 120, 2400m @ 250, yoyos to 50 m.

