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Firmware Release Notes




OEM/NAV

Date:

October 13, 2003

Product:
Ashtech DG16/DG14 OEM Board and Sensor

Subject: 
Firmware Version DC03

Number:  DG2003-02  


Introduction:

     DC03 is a no-cost firmware upgrade for the Ashtech DG16 and DG14 OEM receiver boards and sensors to replace DC00 DG16/DG14 firmware versions.   DC03 can be downloaded from the firmware/DG16_14 folder on Ashtech FTP site ftp://ftp.thalesnavigation.com.   The WINZIP file DG_DC03.ZIP for DG16/14 receiver board and sensor contains the DC03 firmware, loading instructions and these DC03 firmware release notes.   

Changes and Improvements:

1. Allowed receiver to use only full corrections while in SBAS differential mode.

2. Fixed the problem where the receiver may go into KF dead reckoning mode for no reason while working in SBAS differential mode.

3. Resolved the issue that precluded using some fields when defining the selected format for user-defined messages.  DC03 is only compatible with UDM software version 1.03, which is available in the software folder on our ftp site. 
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