Benthos DS7000 Deckbox SN# 145

RMA #02-325

Description of Failure:

Deckbox will not transmit RS232 data to host computer when in remote mode. Deckbox will however accept RS232 control characters. 

In addition, the dunker transducer cable was entangled in the support ships propellers and cut. The cable termination at the transducer is also showing substantial wear. Please reterminate the transducer.

Any questions can be directed to:

Hans Thomas

MBARI

831-775-1976

hthomas@mbari.org 

