Cruise Information

Date:
Cruise:

Ship:
Vehicle Configuration:

Vehicle Pre-Launch Checklist


Launch Coordinator:____________________

Item
Reading/Value
Initials

Battery Sphere Sealed (3-5 PSI Vacuum)



MVC Sphere Sealed (3-5 PSI Vacuum)



Main Battery Voltage



USBL Beacon On



USBL Beacon Voltage



USBL Transmit/Receive Frequency



RDF/Strobe On



RDF Frequency/Channel (C=160.725/D=160.785)



RDF/Strobe Battery Voltage



Propeller Set Screws Tight



Forward & Aft Jbox Compensation Pressure (3-5 PSI)



Compensation Pressure/Height (verify valve open)



Payload Pre-Launch Checklist


Payload Coordinator:____________________

Item
Reading/Value
Initials

DCON Compensation Pressure (3-5 PSI OK)



Optical Backscatter Cap Removed



Hydroscat Cap Removed



CTD 1  - Temperature & Salinity



CTD 2 – Temperature & Salinity



Hydroscat 2 Operational (External Lights & Software)



LISST  Operational (Pump & Software)



Biolume Operational (Pump & Software)



ISUS Operational ( Software)



Confirm $AUV_CONFIG_DIR/devices.cfg correct



Vehicle Pre-Dive Checklist


Pre-Dive Coordinator:_________________

Item
Reading/Value
Initials

Elevator & Rudder Actuators Full Range



Thruster Operational



DVL Operational



Parosci (note temperature



GPS (note fix/no fix)



MVC Date & Time



PS8000/LBL



Metrabyte Battery Voltage & Current



Crossbow



Vehicle Post-Dive Checklist


Post-Dive Coordinator:__________________

Item
Reading/Value
Initials

USBL Beacon Off



RDF/Strobe Off



Vehicle Freshwater Rinse



LISST Flush



Bathyphotometer Flush



HS2 Rinse



CTD1 & CTD2 Flush



Dorado AUV Mission Checklist








