


Dorado AUV Nose Hull Section


LOA = 40.0 in/ 1.106 m


Max mass = 168 kg


CG Location = 24.53 in/ 0.623 m from tip of nose





Dorado AUV Tail Hull Section


LOA = 50.35 in/ 1.279 m


Max mass = 222 kg


CG location = 20.63 in/ 0.524 m from forward edge of section





Dorado AUV Minimum Length Configuration


Primary Mission = CTD survey


Midbody length = 25 in/ 0.635 m


LOA = 115.35 in/ 2.930 m


Max mass = 537 kg


CG location = 57.1 in/ 1.452 m from tip of nose 





Dorado AUV Minimum Length Configuration Extended


Primary Mission = Bioluminescence/LISST survey


Midbody length = 46 in/ 1.168 m


LOA = 136.35 in/ 3.460 m


Max mass = 659 kg


CG location = 67.6 in/ 1.718 m from tip of nose 





Dorado AUV Multibeam Mapping Configuration


Primary Mission = Mapping survey 


Midbody length = 74 in/ 1.880 m


LOA = 164.35 in/ 4.175 m


Max mass = 821 kg


CG location = 81.6 in/ 2.072 m from tip of nose 





Dorado AUV Maximum Length Configuration


Primary Mission = Extended duration/remote data transfer 


Midbody length = 132 in/ 3.353 m


LOA = 222.35 in/ 5.648 m


Max mass = 1159 kg


CG location = 110.5 in/ 2.807 m from tip of nose 


