Mapping AUV Project Meeting

Nose and Midbody PDR

8 April 2003

Attending:

Dave Caress, Paul McGill, Mark Sibenac, Hans Thomas, Andy Hamilton,  Farley Shane, Rob McEwen,  Bill Kirkwood, Paul Chandler

Farley presents the nose section .


Removable front part of nose section.


Recovery hook has to be up front to be the same as the CTD ve.


Bill questions cost/benefit of using removable Bluefin nose cap.


Action Items:



Decide on removable nose – yes, we keep it.



Look at replacing screws holding foam up front with rods.

Recovery hook to be fixed, not removable.



Compensator volume to be increased.



Calculate CG/CB and overall buoyancy.



Remove stiffening rod at rear of section.



Check if we need to move two connectors from side to front of junction box.



Allow for trim weights.

Andy presents the midbody.


Action Items:



Desire to allow for getting into sonar pressure housing 

without disconnecting cables. Rotate it to vertical?



Flare out foam around Edgetech subbottom projector?



Optimize cabling for minimum length, particularly the 

multibeam transmitter cable.



Define cable channels in both upper and lower foam blocks.



Need door for access for front of pressure vessel to 

connect data and disconnect battery.



Allow for trim weights.

Rob – assess penalty of tail dropweight for powered ascent


Powered ascent should work 

– could be used as an ascent dropweight for deep missions.

Sib – Reson I/O module requirements

