Mapping AUV Project Meeting

31 March 2004

Attending:

Dave Caress, Farley Shane, Rob McEwen, Hans Thomas, Bill Kirkwood, Paul McGill, Mark Sibenac

1. Congratulations to Hans on his new position as DMO AUV Group Leader – effective April 14.

2. Vehicle testing  - four Zephyr days during week of April 12-16.

a. Mooring maintenance will occur one day that week – now scheduled for Wednesday but Mike Kelley will choose which day they go.

3. Nose

a. Cart modified to fit better.

b. Ballast test in tank with midbody last week – very buoyant.

c. Ready to go to sea for testing.

d. One screw doesn’t engage by seam – Farley will work on it.

4. Midbody

a. I/o board in from Reson – not installed and we won’t use it for initial tests.

b. Need to make wet cable from Kearfott to Reson housing before the multibeam delivery in May – will  measure and order soon.

c. Ready to go to sea for first tests.

5. Tail

a. Measured out wet cabling lengths

i. Kearfott whip is ready to be molded – soldered and tested - Hans

ii. Parosci whip still needs to be cut – McGill & McEwen - highest priority.

iii. Transducer whip is measured only- McGill & McEwen

iv. USBL whip is measured only – McGill & McEwen

v. Novatech /strobe/drop weight whip is measured only - Kirkwood

vi. Kearfott-GPS needs making too – put off to last

b. New MVC buss-forward whip due back from Seacon on Thursday – replaces cable they built incorrectly.

c. Mark is working on MVC internal wiring – has complete diagrams.

d. Base bracket for MVC electronics made and installed.

e. Will now start stuffing electronics into sphere

f. Need more EMI materials – unable to find oval copper braid in stock at electronics houses. Also need to order copper sheet. McGill.

g. Need to check gearbox and put oil back in tailcone – Farley + Hans.

h. Need two more holes in top faring for antennas and access door in bottom faring.

i. Software

i. Environmental  sensor driver close to done – Rob

ii. Rich writing Reson behavior /driver code .

1. Rob will check status of A-comms driver

2. Also need to start testing Reson commands as soon as possible.

iii. Caress still working on MB-System i/o module for Reson 7k data.

6. Batteries

a. Battery 56 needs fuse replaced.

b. Cobalt battery needs charging – use same profile as for Valence batteries.

