Mass properties of MapHousing

Output  coordinate System : -- default --

Density = 0.17 pounds per cubic inch

Mass = 110.44 pounds

Volume = 653.47 cubic inches

Surface area = 1483.48 square inches

Center of mass: ( inches )


X = 5.75


Y = 0.00


Z = 0.00

Principal axes of inertia and principal moments of inertia: ( pounds * square inches )

Taken at the center of mass.


 Ix = (1.00, 0.00, 0.00)   
Px = 4010.38


 Iy = (0.00, 1.00, 0.00)   
Py = 4793.81


 Iz = (0.00, 0.00, 1.00)   
Pz = 4793.81

Moments of inertia: ( pounds * square inches )

Taken at the center of mass and aligned with the output coordinate system.


Lxx = 4010.38
Lxy = 0.00
Lxz = 0.00


Lyx = 0.00
Lyy = 4793.81
Lyz = 0.00


Lzx = 0.00
Lzy = 0.00
Lzz = 4793.81

Moments of inertia: ( pounds * square inches )

Taken at the output coordinate system.


Ixx = 4010.38
Ixy = 0.00
Ixz = 0.00


Iyx = 0.00
Iyy = 8444.62
Iyz = 0.00


Izx = 0.00
Izy = 0.00
Izz = 8444.62

