Mass properties of Mapping PV revB

Output  coordinate System : -- default --

Density = 0.169 pounds per cubic inch

Mass = 21.622 pounds

Volume = 127.943 cubic inches

Surface area = 537.452 square inches

Center of mass: ( inches )


X = 0.000


Y = 1.894


Z = 0.006

Principal axes of inertia and principal moments of inertia: ( pounds * square inches )

Taken at the center of mass.


 Ix = (0.707, 0.001, 0.707)   
Px = 370.227


 Iy = (0.707, -0.001, -0.707)   
Py = 370.227


 Iz = (-0.000, 1.000, -0.001)   
Pz = 579.358

Moments of inertia: ( pounds * square inches )

Taken at the center of mass and aligned with the output coordinate system.


Lxx = 370.227
Lxy = 0.001
Lxz = -0.000


Lyx = 0.001
Lyy = 579.358
Lyz = 0.304


Lzx = -0.000
Lzy = 0.304
Lzz = 370.227

Moments of inertia: ( pounds * square inches )

Taken at the output coordinate system.


Ixx = 447.781
Ixy = 0.002
Ixz = -0.000


Iyx = 0.002
Iyy = 579.359
Iyz = 0.538


Izx = -0.000
Izy = 0.538
Izz = 447.781

