ACAD FILE: 11391p4.DWG 8

A

B

7 6 5

C

D

8 7 6 5

4 3 2 1

A

B

4 ZONE LTR 3

C

APPROVED

REVISIONS

DESCRIPTION DATE 2 1

D

0.005/0.010 0.005/0.010

TOLERANCES DO NOT SCALE DRAWING DIMENSIONS ARE IN INCHES UNLESS OTHERWISE SPECIFIED

- NEXT ASSY USED ON

APPLICATION 7K INTERNAL RADII BREAK CORNERS REMOVE ALL BURRS

X° ±0.5° .XXX ±0.010 .XX ±0.03

DRAWING NO: D

DRAWN

DATE:

SIZE:

TITLE:

THALES AUV

SYSTEM BLOCK DIAGRAM,

11391

SCALE: NONE 1

SHEET: 1OF P5 REV:

ANSI-D.DWG REV A

DATE:

DESIGNED:

DATE:

CHECKED

DATE:

RELEASED

THIRD ANGLE PROJECTION RESON, INC.

GOLETA, CALIFORNIA 93117 GJZ

NOTICE OF PROPRIETARY RIGHTS

OR USED FOR MANUFACTURING OR ANY OTHER PURPOSE WITHOUT PRIOR REPRODUCED OR TRANSFERED TO DOCUMENTS OR DISCLOSED TO OTHERS THIS DOCUMENT CONTAINS PROPRIETARY INFORMATION IT MAY NOT BE

NOTES: UNLESS OTHERWISE SPECIFIED

WRITTEN PERMISSION

-

P PRELIMINARY 01-07-10

01-07-10 R. ABBOTT

RQA

01-07-10

01-07-10 R. ABBOTT

4 TP ba tte ry JBOX

SSS STBD

MBE TX

LOAD & PROCESSING

SSS PORT

SHIP BOARD

DATA DOCKING

SYSTEM, DATA OFF

4 TP

22 1

6 5 22 22 3 4 2 22 22 22 DESCRIPTION AWG PIN 2 MHDL-16-BCR

7 6 BCR 1506F

22 12

9 11 10 22 22 22 7 8 22 22

13 20

16 15 14 20 20 20

20 16

9 22

15 14 13 20 20 20 12 11 10 22 22 22

22 6 8 7 22 22

3 5 4 22 22 22

MHDL-16-BCR

DESCRIPTION AWG 8 PIN 1 2 22 22

6 16 8 7 16 16

4 5 3 22 16 22

DESCRIPTION BCR1508F 5

2 PIN 1 22 22 AWG

TXL -

TXH - TXH +

TXL +

DESCRIPTION

22 5 4 22 3 2 22 22 AWG PIN 1 22

6 22

BCR 1505F

DESCRIPTION 22 22 22 22 5 4 3 2 22 AWG PIN 1

SBP

HF- LF+ LF-

SHIELD HF+ Tx + SHIELD

Tx -

Rx - Rx +

Rx SHIELD

ETHERNET RJ45 PIN 1

BATT BUS +V

BATT BUS 0V

BATT BUS +V BATT BUS 0V SHIELD/CHASSIS

ETHERNET RJ45 PIN 2

ETHERNET RJ45 PIN 3

ETHERNET RJ45 PIN 4

SHIELD/CHASSIS

ETHERNET RJ45 PIN 4

ETHERNET RJ45 PIN 3

BATT BUS 0V

BATT BUS 0V

BATT BUS +V

BATT BUS +V

ETHERNET RJ45 PIN 2

ETHERNET RJ45 PIN 1

8

7

PRESSURE PAYLOAD

VESSEL

6

5

4

2

3

1

MBE RX

SBP SSS PORT

MEH CONNECTION

SHORE CONNECTION MBE Tx

LNK 1B- LNK 1B+ LNK 1A- LNK 1A+

DVL/INS

SSS STBD

SHIELD HF+ HF- LF+ LF-

3 DESCRIPTION

22 5 22 4 22 3 22 2 22 1 PIN AWG FCR1509F

Ena ble

Ena ble Rtn

Obs Sona r RS232 TX to Re son CTD TX to Re son

+12V Inst Pwr

Obs Sona r Sync

+12V Inst Pwr Rtn

CTD

Obs Sona r

DVL Trigge r INS/GPS 1PPS Out INS RS232 RX fr Re son INS RS232 TX to Re som

INS/GPS Rtn

Se a de vil Comms 4 22 22 22 1 3 2 22 22 22 4 5 6 22 8 7 22

DESCRIPTION PIN AWG BCR 1508F

BCR1508M AWG PIN DESCRIPTION

+12V 16 7 COM 8 16 6 5 4 16 16 22 2 3 1 22 22 22 1 MBE Rx

LNK 1C+

LNK 1C-

LNK 1A+

LNK 1A-

LNK 1B+

LNK 1B-