Dorado AUV Mission Checklist

Date: ______________________ 
Cruise: ________________________

Ship: ______________________
Vehicle: _______________________

Pre Launch Checks

                                                                                                                                                              Initials
Spheres Sealed  Forward_______   Aft _______     (3-5 PSI Vacuum)                     _____

Main Battery Charged    _______ V (Min = 50.0)                                                     _____

USBL Beacon Charged  _______ V (Min = 14.0)                                                     _____

USBL RX/TX                 ___/___ kHz                                                                       _____

RDF TX                          _______ (C=160.725/D=160.785MHz)                             _____

RDF Batteries                 _______V (Min = 6.0)                                                        _____

Strobe Batteries              _______V (Min = 6.0)                                                        _____

USBL Beacon ON          _______                                                                              _____

RDF                ON           _______                                                                              _____

Strobe             ON           _______                                                                              _____



Launch Coordinator: ________________________

Pre Dive Checks

Vehicle Checks

                 Initials                                                                                                    Initials

Actuators     _____                                                                               Fins Indexed   _____

Thruster       _____                                                                               Time Sync       _____

DVL            _____                                                                                PS8000           _____

ParoSci        _____                                                                                Altimeter        _____

CTD            _____                                                                                Crossbow       _____

GPS             _____                                                                                Fuel Cell        _____

Mission Configured and Simulated _____





Surface Controller: __________________________

Post Dive Checks

                                         Initials                                                                             Initials

USBL Beacon OFF         _____                                                    Strobe OFF        _____

RDF                OFF         _____                                           Fresh Water Rinse       _____

Data Files Downloaded    _____



