ElmoPWM PCB Modification (S/N 004)

Dorado 600024 – sib x2028

Cut pins close to ElmoPWMR2 PCB for M3,M2,M1,VP+,VP-

Desolder and put out stubbies on M3,M2,M1,VP+,VP-

Cuts J1, J2, J3 pins down far enough to drop the clearance between the top two boards

Trim pins on PLB16M4BN0A1 connector to get more clearance around that PLCC chip

Solder M3, M2, M1, VP+, VP- pins back onto ElmoPWMR2 PCB

