GFDetector #1 A/D Conversion

Power Common Leakage.  Microamps = (Ch.0 count-248) / -2.439

(code 01)

Battery + Leakage.             Microamps = (Ch.0 count-248) / 2.439

(code 11)

Battery Voltage.                  Volts = (Ch.1 count) / 251.4

GFDetector #2 A/D Conversion

Power Common Leakage.  Microamps = (Ch.0 count-250) / -2.492

(code 01)

Battery + Leakage.             Microamps = (Ch.0 count-247) / 2.494

(code 11)

Battery Voltage.                  Volts = (Ch.1 count) / 251

