ASIMET BPR
1. Device initialization performed by instrument service

None
2. Device metadata returned in SIAM datastream
BPR01

BPR222

VOSBPR53 v3.3(Heise)

2.4576 Mhz

17NOV05

2006/03/17  17:37:10

BPR:  0.00000e+00  1.00000e+00

No PCMCIA card installed

MODADR: BPR01

MODMFG: Star Eng.

MODMOD: VOSBPR

MODSER: BPR222

MODDAT: 09SEP05

SENMFG: DRESSER

SENMOD: DXD

SENSER: 2935

SENDAT: 2005

SFTMFG: WHOI/GEOFF

SFTNAM: VOSBPR53

SFTREV: 3.3

SFTDAT: 12JUN02

CALFAC: WHOI

CALPER: J.C.SMITH

CALDAT: 17NOV05

DATFRM: -

DATDES: -

DATUNI: -

RAWFRM: -

RAWDES: -

RAWUNI: -

3. Instrument-specific service properties
/** Must be LWR, SWR, WND, HRH, or BPR */

String sensorType;

/** Instrument module address – “01”, “02”, etc. */

String moduleAddress;

4. Initial service property values for this deployment
powerPolicy=ALWAYS

commPowerPolicy=SAMPLING

currentLimitMa=2000

nominalCurrentMa=1000

powerOnDelaySec=0

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

maxSampleTries=3

sampleTimeoutMsec=3000

startDelayMsec=4000

sensorType=BPR
moduleAddress=01

5. Results of acceptance test procedures
OK
6. Known-service bugs/deficiencies
None







