ASIMET HRH
1. Device initialization performed by instrument service

None
2. Device metadata returned in SIAM datastream
Requesting cal constants - OK

HRH01

HRH355

VOSHRH53 v3.2

2.4576 Mhz

14JUL05

2006/03/17  14:15:17

RH%:  8.59030e+02 -7.72235e-02  2.15980e-06 -1.82900e-11

RHT: -2.91250e+02  7.65420e-03  0.00000e+00  0.00000e+00

No PCMCIA card installed

MODADR: HRH01

MODMFG: STAR ENG

MODMOD: VOSHRH

MODSER: HRH355

MODDAT: 30OCT03

SENMFG: ROTRONIC

SENMOD: MP101A

SENSER: R93858

SENDAT: 28OCT03

SFTMFG: WHOI/GEOFF

SFTNAM: VOSHRH53

SFTREV: 3.2

SFTDAT: 12JUN02

CALFAC: WHOI

CALPER: J.C.SMITH

CALDAT: 14JUL05

DATFRM: -

DATDES: -

DATUNI: -

RAWFRM: -

RAWDES: -

RAWUNI: -

3. Instrument-specific service properties
/** Must be LWR, SWR, WND, HRH, or BPR */

String sensorType;

/** Instrument module address – “01”, “02”, etc. */

String moduleAddress;

4. Initial service property values for this deployment
powerPolicy=ALWAYS

commPowerPolicy=SAMPLING

currentLimitMa=2000

nominalCurrentMa=1000

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

maxSampleTries=3

powerOnDelaySec=0

sampleTimeoutMsec=3000

startDelayMsec=4000

sensorType=HRH

moduleAddress=01

5. Results of acceptance test procedures
OK
6. Known-service bugs/deficiencies
None







