ASIMET WND
1. Manually-configured instrument settings not handled by service
None.

2. Device metadata returned in SIAM datastream
WND01

WND358

VOSWND53 v3.5

2.4576 Mhz

22JUL05

2006/03/17  15:13:30

No PCMCIA card installed

MODADR: WND01

MODMFG: STARENG.

MODMOD: VOSWND

MODSER: WND358

MODDAT: 29JUL03

SENMFG: USD/PNAV

SENMOD: A2-S-B/-

SENSER: 9241/87

SENDAT: -

SFTMFG: WHOI/GEOFF

SFTNAM: PICWND

SFTREV: V1.5

SFTDAT: -

CALFAC: WHOI

CALPER: J.C.SMITH

CALDAT: 22JUL05

DATFRM: -

DATDES: -

DATUNI: -

RAWFRM: -

RAWDES: -

RAWUNI: -

3. Instrument-specific service properties
/** Must be LWR, SWR, WND, HRH, or BPR */

String sensorType;

/** Instrument module address – “01”, “02”, etc. */

String moduleAddress;

4. Initial service property values for this deployment
powerPolicy=ALWAYS

commPowerPolicy=SAMPLING

currentLimitMa=2000

nominalCurrentMa=1000

powerOnDelaySec=0

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

maxSampleTries=3

sampleTimeoutMsec=3000

startDelayMsec=4000

sensorType=WND
moduleAddress=01

5. Results of acceptance test procedures
OK
6. Known-service bugs/deficiencies
None







