WETLabs ECO FLNTU
1. Device initialization performed by instrument service
Sets average per sample, samples per packet, packets per set, interval between packets, packet interval; enables or disables internal logging.
2. Device metadata returned in SIAM datastream
Ver FLNTUS 2.70 

Ave 20 Pkt 5 

Set 1 

Rec 1 

Int 00:00:05 

Dat 03/17/06 

Clk 04:10:32 

Mem 3512

3. Instrument-specific service properties
/** Number of measurements in each sample ("$ave") */

int averageCount = 50;

/** Number of samples in a packet ("$pkt"). */

   int samplesPerPacket = 3;

/** Number of times to repeat packet ("$set") */

int packetsPerSet = 1;

/** Interval between packets - must be expressed as hh:mm:ss */

String packetInterval = "0:0:0";

/** Enable or disable data logging to instrument FLASH. */

boolean logEnabled = true;

4. Initial service property values for this deployment
powerPolicy=ALWAYS 

commPowerPolicy=SAMPLING 

powerOnDelaySec=0 

nominalCurrentMa=1000 
currentLimitMa=1000 

sampleSchedule=R */0 */10 */0 */0 * * * * GMT * 

maxSampleTries=3 

sampleTimeoutMsec=60000 

packetsPerSet=1 

serviceStatus=2 

averageCount=20 

startDelayMsec=2000 

samplesPerPacket=5
logEnabled=true 

5. Results of acceptance test procedures
OK
6. Known-service bugs/deficiencies
None







