testport.sh node21 /dev/ttySX0

node=//node21/node

port=/dev/ttySX0

SIAM version $Name: march14_2006 $

Node 1481 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Satlantic HyperOCR s/n 239           1517    OK        281   0   8

/dev/ttySX1  Seabird-37SM s/n 37SM26805-2004      1277    OK          4   0   0

/dev/ttySX2  Satlantic MBARI ISUS s/n 090         1514    OK         46   1   1

/dev/ttySX3  Garmin GPS s/n 81106809              1504    OK          4   0   0

/dev/ttySX4  ASIMET LWR s/n LWR308                1289    OK        281   0   0

/dev/ttySX5  Seahorse Profiler s/n 10322          1405    ERROR       0 240 792

/dev/ttySX6  -                                    -       -        -           

/dev/ttySX7  -                                    -       -        -           

/dev/ttySX8  -                                    -       -        -           

/dev/ttySX9  -                                    -       -        -           

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 MSP430 (sidearm4.21)                 1483    OK       3062   0   0

/dev/ttySA2  Medusa card s/n 2.004                1442    OK          7   0   0

Press any key to sample instrument on port  /dev/ttySX0 :

number of args: 2

SIAM version $Name: march14_2006 $

Satlantic HyperOCR s/n 239:

parentID=1481, recordType=1

devid=1517, t=1142565560720, seqNo=435, mdref=154

nBytes=4354

SATHSE0239*****u*******************************

Parser not implemented.
Press any key to get most recent sample from instrument on port  /dev/ttySX0 :

SIAM version $Name: march14_2006 $

parentID=1481, recordType=1

devid=1517, t=1142565560720, seqNo=435, mdref=154

nBytes=4354

SATHSE0239*****u*******************************

Press any key to shutdown service on port  /dev/ttySX0 :

SIAM version $Name: march14_2006 $

Shutdown port /dev/ttySX0

OK

SIAM version $Name: march14_2006 $

Node 1481 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  -                                    -       -        -           

/dev/ttySX1  Seabird-37SM s/n 37SM26805-2004      1277    OK          5   0   0

/dev/ttySX2  Satlantic MBARI ISUS s/n 090         1514    OK         46   1   1

/dev/ttySX3  Garmin GPS s/n 81106809              1504    OK          4   0   0

/dev/ttySX4  ASIMET LWR s/n LWR308                1289    OK        282   0   0

/dev/ttySX5  Seahorse Profiler s/n 10322          1405    ERROR       0 240 792

/dev/ttySX6  -                                    -       -        -           

/dev/ttySX7  -                                    -       -        -           

/dev/ttySX8  -                                    -       -        -           

/dev/ttySX9  -                                    -       -        -           

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 MSP430 (sidearm4.21)                 1483    OK       3068   0   0

/dev/ttySA2  Medusa card s/n 2.004                1442    OK          8   0   0

Should now be no service on port  /dev/ttySX0
Press any key to load service on port  /dev/ttySX0 :

SIAM version $Name: march14_2006 $

Scan port /dev/ttySX0

SIAM version $Name: march14_2006 $

Node 1481 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Satlantic HyperOCR s/n 239           1517    OK          0   0   0

/dev/ttySX1  Seabird-37SM s/n 37SM26805-2004      1277    OK          5   0   0

/dev/ttySX2  Satlantic MBARI ISUS s/n 090         1514    OK         46   1   1

/dev/ttySX3  Garmin GPS s/n 81106809              1504    OK          5   0   0

/dev/ttySX4  ASIMET LWR s/n LWR308                1289    OK        282   0   0

/dev/ttySX5  Seahorse Profiler s/n 10322          1405    ERROR       0 240 792

/dev/ttySX6  -                                    -       -        -           

/dev/ttySX7  -                                    -       -        -           

/dev/ttySX8  -                                    -       -        -           

/dev/ttySX9  -                                    -       -        -           

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 MSP430 (sidearm4.21)                 1483    OK       3071   0   0

/dev/ttySA2  Medusa card s/n 2.004                1442    OK          8   0   0

Should now be service running on port  /dev/ttySX0
Press any key to get instrument metadata from port  /dev/ttySX0 :

Looking for node server stub at rmi://node21/node

Got proxy for node service "moos.deployed.NodeService"

Requesting packet...components = 0x1f

Packet received:

parentID=1481, recordType=0

devid=1517, t=1142565883061, seqNo=0, mdref=0

 cause=just checking

<DEV_MD>

MASTER NODE:

ID:

id

HyperOCR - Hyperspectral Ocean Colour Radiometer

Copyright (C) 2004, Satlantic Inc. All rights reserved.

Firmware version: 1.2B(P), 1.0A(S) - SatNet Type A

Instrument: SATHSE

S/N: 0239

[Auto]

STATE:

show all

Telemetry Baud Rate: 57600 bps

Maximum Frame Rate: AUTO

Initialize Silent Mode: off

Initialize Power Down: off

Initialize Automatic Telemetry: on

Network Mode: off

Network Address: 150

Network Baud Rate: 38400 bps

Network Master Mode: off

Master Controlled Telemetry: off

Master Network Bias: on

Network Reset Delay: 5

Minimum Integration Time: 8 ms

Maximum Integration Time: 2048 ms

Starting Integration Time: 128 ms

Increase Factor: 2.000000

Decrease Factor: 0.500000

Adaptive Gain: on

Upper Threshold: 42000

Lower Threshold: 10000

Dark Frames: 5

[Auto]

</DEV_MD>

<SRVC_MD>

powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.ocr3000.Ocr3000$Attributes

serviceName=Satlantic HyperOCR s/n 239

parentID=1481

currentLimitMa=8000

sampleSchedule=A */0 */10 */0 */0 * * * * GMT *

extendedVersion=UNK

frameworkVersion=$Name: march14_2006 $

UUID=bd01ceec-a3f8-11da-bb39-00306e389969

powerPolicy=SAMPLING

timeSynch=false

maxSampleTries=3

isiID=1517

sampleTimeoutMsec=1000

commPowerPolicy=SAMPLING

serviceStatus=0

sampleTime=30000 **(amt of time data collected from OCR-3000)
startDelayMsec=10000

</SRVC_MD>

<DOC_MD>

unable to access XML file

</DOC_MD>

Press any key to show schedule for instrument on  /dev/ttySX0 :

ShowSchedule: lookAhead value undefined or invalid; using default (3600)

Looking for node service at rmi://node21/node

Got proxy for node service "moos.deployed.NodeService"

    Name: Default

   Owner: moos.devices.ocr3000.Ocr3000:1517 key=14

Schedule: A */0 */10 */0 */0 * * * * GMT *

  Status: Waiting
302000

Test complete.

node21:/mnt/hda/siam/atp$ 

