node=//surface/node

port=/dev/ttySX1

SIAM version $Name: march14_2006 $

Node 1446 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Mooring power can s/n 002            1322    OK          1   1   3

/dev/ttySX1  Snubber Node Power Control           1502    OK          1   0   0

/dev/ttySX2  -                                    -       -        -           

/dev/ttySX3  -                                    -       -        -           

/dev/ttySX4  ASIMET BPR s/n BPR222                1443    OK          2   0   0

/dev/ttySX5  MBARI pCO2 s/n SOON1S                1448    ERROR       0   1   0

/dev/ttySX6  Triaxys s/n TAS01020                 1286    SLEEPING    0   0   0

/dev/ttySX7  ASIMET HRH s/n HRH355                1290    OK          2   0   0

/dev/ttySX8  ASIMET WND s/n WND358                1291    SAMPLING    1   0   0

/dev/ttySX9  ASIMET SWR s/n SWR344                1292    OK          1   0   0

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 -                                    -       -        -           

/dev/ttySA2  -                                    -       -        -           

Press any key to sample instrument on port  /dev/ttySX1 :

number of args: 2

SIAM version $Name: march14_2006 $

Snubber Node Power Control:

parentID=1446, recordType=1

devid=1502, t=1142568284862, seqNo=77, mdref=76

nBytes=2

**

Parser not implemented.
Press any key to get most recent sample from instrument on port  /dev/ttySX1 :

SIAM version $Name: march14_2006 $

parentID=1446, recordType=1

devid=1502, t=1142568284862, seqNo=77, mdref=76

nBytes=2

**
Press any key to shutdown service on port  /dev/ttySX1 :

SIAM version $Name: march14_2006 $

Shutdown port /dev/ttySX1

OK

SIAM version $Name: march14_2006 $

Node 1446 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Mooring power can s/n 002            1322    OK          1   1   3

/dev/ttySX1  -                                    -       -        -           

/dev/ttySX2  -                                    -       -        -           

/dev/ttySX3  -                                    -       -        -           

/dev/ttySX4  ASIMET BPR s/n BPR222                1443    OK          2   0   0

/dev/ttySX5  MBARI pCO2 s/n SOON1S                1448    ERROR       0   1   0

/dev/ttySX6  Triaxys s/n TAS01020                 1286    SLEEPING    0   0   0

/dev/ttySX7  ASIMET HRH s/n HRH355                1290    OK          2   0   0

/dev/ttySX8  ASIMET WND s/n WND358                1291    OK          2   0   0

/dev/ttySX9  ASIMET SWR s/n SWR344                1292    OK          1   0   0

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 -                                    -       -        -           

/dev/ttySA2  -                                    -       -        -           

Should now be no service on port  /dev/ttySX1

Press any key to load service on port  /dev/ttySX1 :

SIAM version $Name: march14_2006 $

Scan port /dev/ttySX1

SIAM version $Name: march14_2006 $

Node 1446 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Mooring power can s/n 002            1322    OK          1   1   3

/dev/ttySX1  Snubber Node Power Control           1502    OK          1   0   0

/dev/ttySX2  -                                    -       -        -           

/dev/ttySX3  -                                    -       -        -           

/dev/ttySX4  ASIMET BPR s/n BPR222                1443    OK          2   0   0

/dev/ttySX5  MBARI pCO2 s/n SOON1S                1448    ERROR       0   1   0

/dev/ttySX6  Triaxys s/n TAS01020                 1286    SLEEPING    0   0   0

/dev/ttySX7  ASIMET HRH s/n HRH355                1290    OK          2   0   0

/dev/ttySX8  ASIMET WND s/n WND358                1291    OK          2   0   0

/dev/ttySX9  ASIMET SWR s/n SWR344                1292    OK          1   0   0

/dev/ttySX10 Workhorse LR ADCP 300kHz s/n 4164    1294    SAMPLING    0   0   0

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 -                                    -       -        -           

/dev/ttySA2  -                                    -       -        -           

Should now be service running on port  /dev/ttySX1
Press any key to get instrument metadata from port  /dev/ttySX1 :

Looking for node server stub at rmi://surface/node

Got proxy for node service "moos.deployed.NodeService"

Requesting packet...components = 0x1f

Packet received:

parentID=1446, recordType=0

devid=1502, t=1142568347893, seqNo=0, mdref=0

 cause=just checking

<DEV_MD>

Snubber Node Power Control does not provide instrument state information

</DEV_MD>

<SRVC_MD>

powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=org.mbari.isi.interfaces.InstrumentServiceAttributes

serviceName=Snubber Node Power Control

parentID=1446

currentLimitMa=12000

sampleSchedule=R */0 */0 */1 */0 * * * * GMT *

extendedVersion=UNK

frameworkVersion=$Name: march14_2006 $

UUID=63623646-8d28-11da-92c6-00306e389969

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=1

isiID=1502

sampleTimeoutMsec=1000

commPowerPolicy=NEVER

serviceStatus=0

startDelayMsec=0

</SRVC_MD>

<DOC_MD>

unable to access XML file

</DOC_MD>

Press any key to show schedule for instrument on  /dev/ttySX1 :

ShowSchedule: lookAhead value undefined or invalid; using default (3600)

Looking for node service at rmi://surface/node

Got proxy for node service "moos.deployed.NodeService"

    Name: Default

   Owner: moos.devices.powerswitch.PowerSwitch:1502 key=11

Schedule: R */0 */0 */1 */0 * * * * GMT *

  Status: Waiting
3560405

Test complete.

surface:/mnt/hda/siam/atp$ 

