Snubber Node Power Switch
(Surface Node(1446), Port 1, ISI-ID = 1502
1. Instrument device settings initialized by SIAM service. 
None.
2. Device metadata returned in SIAM datastream
parentID=1446, recordType=0

devid=1502, t=1142568347893, seqNo=0, mdref=0

 cause=just checking

Snubber Node Power Control does not provide instrument state information
3. Instrument-specific service properties
None.

4. Initial service property values for this deployment
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=org.mbari.isi.interfaces.InstrumentServiceAttributes

serviceName=Snubber Node Power Control

parentID=1446

currentLimitMa=12000

sampleSchedule=R */0 */0 */1 */0 * * * * GMT *

extendedVersion=UNK

frameworkVersion=$Name: march14_2006 $

UUID=63623646-8d28-11da-92c6-00306e389969

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=1

isiID=1502

sampleTimeoutMsec=1000

commPowerPolicy=NEVER

serviceStatus=0

startDelayMsec=0
5. Results of acceptance test procedures
All OK.
6. Known-service bugs/deficiencies
unable to access XML file







