WHOI ASIMET SWR
(Surface Node(1446), Port 9, ISI-ID = 1292)
1. Instrument device settings initialized by SIAM service. 
None.
2. Device metadata returned in SIAM datastream
parentID=1446, recordType=0

devid=1292, t=1142568018442, seqNo=0, mdref=0

 cause=just checking

Requesting cal constants - OK

SWR01
SWR344

VOSSWR53 v3.3
2.4576 Mhz
15AUG05
2006/03/17  04:03:40
SWR: -3.98472e+03  1.21790e-01  0.00000e+00  0.00000e+00
No PCMCIA card installed

MODADR: SWR01
MODMFG: STAR ENG
MODMOD: VOSSWR
MODSER: SWR344
MODDAT: 24OCT03
SENMFG: EPPLEY
SENMOD: PSP
SENSER: 33677F3
SENDAT: 27FEB03
SFTMFG: WHOI/GEOFF
SFTNAM: VOSSWR53
SFTREV: 3.3
SFTDAT: 26NOV03
CALFAC: WHOI
CALPER: J.C.SMITH
CALDAT: 15AUG05
DATFRM: -
DATDES: -
DATUNI: -
RAWFRM: -
RAWDES: -
RAWUNI: -

3. Instrument-specific service properties
moduleAddress=01

sensorType=SWR

4. Initial service property values for this deployment
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.asimet.WhoiAsimet$Attributes

serviceName=ASIMET SWR s/n SWR344

parentID=1446

currentLimitMa=2000

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

extendedVersion=UNK

frameworkVersion=$Name: march14_2006 $

UUID=FC5BD33E-E7D6-4CF8-9A17-944A175A2B39

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=3

isiID=1292

sampleTimeoutMsec=3000

commPowerPolicy=SAMPLING

serviceStatus=0

startDelayMsec=4000

5. Results of acceptance test procedures
All Okay.

6. Known-service bugs/deficiencies
unable to access XML file







