testport.sh node21 /dev/ttySX4

node=//node21/node

port=/dev/ttySX4

SIAM version $Name: march14_2006 $

Node 1481 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Satlantic HyperOCR s/n 239           1517    OK          0   0   0

/dev/ttySX1  Seabird-37SM s/n 37SM26805-2004      1277    OK          5   0   0

/dev/ttySX2  Satlantic MBARI ISUS s/n 090         1514    OK         46   1   1

/dev/ttySX3  Garmin GPS s/n 81106809              1504    OK          5   0   0

/dev/ttySX4  ASIMET LWR s/n LWR308                1289    OK        282   0   0

/dev/ttySX5  Seahorse Profiler s/n 10322          1405    ERROR       0 240 792

/dev/ttySX6  -                                    -       -        -           

/dev/ttySX7  -                                    -       -        -           

/dev/ttySX8  -                                    -       -        -           

/dev/ttySX9  -                                    -       -        -           

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 MSP430 (sidearm4.21)                 1483    OK       3073   0   0

/dev/ttySA2  Medusa card s/n 2.004                1442    OK          9   0   0

Press any key to sample instrument on port  /dev/ttySX4 :

number of args: 2

SIAM version $Name: march14_2006 $

ASIMET LWR s/n LWR308:

parentID=1481, recordType=1

devid=1289, t=1142566097367, seqNo=435, mdref=153

nBytes=71

 295.81  295.82  10983.9  10966.8  -79.5  431.7   33284   33402   32751

Parser not implemented.
Press any key to get most recent sample from instrument on port  /dev/ttySX4 :

SIAM version $Name: march14_2006 $

parentID=1481, recordType=1

devid=1289, t=1142566097367, seqNo=435, mdref=153

nBytes=71

 295.81  295.82  10983.9  10966.8  -79.5  431.7   33284   33402   32751
Press any key to shutdown service on port  /dev/ttySX4 :

SIAM version $Name: march14_2006 $

Shutdown port /dev/ttySX4

OK

SIAM version $Name: march14_2006 $

Node 1481 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Satlantic HyperOCR s/n 239           1517    OK          0   0   0

/dev/ttySX1  Seabird-37SM s/n 37SM26805-2004      1277    OK          6   0   0

/dev/ttySX2  Satlantic MBARI ISUS s/n 090         1514    SAMPLING   46   1   1

/dev/ttySX3  Garmin GPS s/n 81106809              1504    OK          5   0   0

/dev/ttySX4  -                                    -       -        -           

/dev/ttySX5  Seahorse Profiler s/n 10322          1405    ERROR       0 240 792

/dev/ttySX6  -                                    -       -        -           

/dev/ttySX7  -                                    -       -        -           

/dev/ttySX8  -                                    -       -        -           

/dev/ttySX9  -                                    -       -        -           

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 MSP430 (sidearm4.21)                 1483    OK       3077   0   0

/dev/ttySA2  Medusa card s/n 2.004                1442    OK         10   0   0

Should now be no service on port  /dev/ttySX4
Press any key to load service on port  /dev/ttySX4 :

SIAM version $Name: march14_2006 $

Scan port /dev/ttySX4

SIAM version $Name: march14_2006 $

Node 1481 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Satlantic HyperOCR s/n 239           1517    SAMPLING    0   0   1

/dev/ttySX1  Seabird-37SM s/n 37SM26805-2004      1277    OK          6   0   0

/dev/ttySX2  Satlantic MBARI ISUS s/n 090         1514    OK         47   1   1

/dev/ttySX3  Garmin GPS s/n 81106809              1504    OK          5   0   0

/dev/ttySX4  ASIMET LWR s/n LWR308                1289    OK          1   0   0

/dev/ttySX5  Seahorse Profiler s/n 10322          1405    ERROR       0 240 792

/dev/ttySX6  -                                    -       -        -           

/dev/ttySX7  -                                    -       -        -           

/dev/ttySX8  -                                    -       -        -           

/dev/ttySX9  -                                    -       -        -           

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 MSP430 (sidearm4.21)                 1483    OK       3083   0   0

/dev/ttySA2  Medusa card s/n 2.004                1442    OK         10   0   0

Should now be service running on port  /dev/ttySX4
Press any key to get instrument metadata from port  /dev/ttySX4 :

Looking for node server stub at rmi://node21/node

Got proxy for node service "moos.deployed.NodeService"

Requesting packet...components = 0x1f

Packet received:

parentID=1481, recordType=0

devid=1289, t=1142566263963, seqNo=0, mdref=0

 cause=just checking

<DEV_MD>

Requesting cal constants - OK

LWR01

LWR308

VOSLWR53 v3.5

2.4576 Mhz

02AUG05

2006/03/17  03:36:16

Set1: -5.74036e+05  1.75140e+01  0.00000e+00  0.00000e+00

Set2:  1.02652e-03  2.39674e-04  1.54012e-07  0.00000e+00

Set3: -5.74083e+05  1.75154e+01  0.00000e+00  0.00000e+00

Set4:  1.03175e-03  2.38963e-04  1.56149e-07  0.00000e+00

Set5: -2.00893e+04  6.10967e-01  0.00000e+00  0.00000e+00

Set6:  3.93300e+02  2.66000e+00  0.00000e+00  0.00000e+00

No PCMCIA card installed

MODADR: LWR01

MODMFG: STARENG.

MODMOD: VOSLWR

MODSER: LWR308

MODDAT: 24OCT03

SENMFG: EPPLEY LAB

SENMOD: PIR

SENSER: 33681F3

SENDAT: -

SFTMFG: WHOI/GEOFF

SFTNAM: VOSLWRF

SFTREV: 1.6

SFTDAT: 26APR04

CALFAC: WHOI

CALPER: J.C.SMITH

CALDAT: 02AUG05

DATFRM: -

DATDES: -

DATUNI: -

RAWFRM: -

RAWDES: -

RAWUNI: -

</DEV_MD>

<SRVC_MD>

moduleAddress=01 **
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.asimet.WhoiAsimet$Attributes

serviceName=ASIMET LWR s/n LWR308

parentID=1481

currentLimitMa=2000

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

extendedVersion=UNK

frameworkVersion=$Name: march14_2006 $

UUID=3dcc5cbb-47ca-11da-950b-00306e389969

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=3

isiID=1289

sampleTimeoutMsec=3000

commPowerPolicy=SAMPLING

serviceStatus=0

startDelayMsec=4000

sensorType=LWR **
</SRVC_MD>

<DOC_MD>

unable to access XML file

</DOC_MD>

Press any key to show schedule for instrument on  /dev/ttySX4 :

ShowSchedule: lookAhead value undefined or invalid; using default (3600)

Looking for node service at rmi://node21/node

Got proxy for node service "moos.deployed.NodeService"

    Name: Default

   Owner: moos.devices.asimet.WhoiAsimet:1289 key=15

Schedule: R */0 */10 */0 */0 * * * * GMT *

  Status: Waiting
544158

Test complete.

node21:/mnt/hda/siam/atp$ 

