node=//surface/node

port=/dev/ttySX9

SIAM version $Name: march14_2006 $

Node 1446 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Mooring power can s/n 002            1322    ERROR       0   1   3

/dev/ttySX1  Snubber Node Power Control           1502    OK          1   0   0

/dev/ttySX2  -                                    -       -        -           

/dev/ttySX3  -                                    -       -        -           

/dev/ttySX4  ASIMET BPR s/n BPR222                1443    OK          1   0   0

/dev/ttySX5  MBARI pCO2 s/n SOON1S                1448    ERROR       0   1   0

/dev/ttySX6  Triaxys s/n TAS01020                 1286    SLEEPING    0   0   0

/dev/ttySX7  ASIMET HRH s/n HRH355                1290    OK          1   0   0

/dev/ttySX8  ASIMET WND s/n WND358                1291    OK          1   0   0

/dev/ttySX9  ASIMET SWR s/n SWR344                1292    OK          1   0   0

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 -                                    -       -        -           

/dev/ttySA2  -                                    -       -        -           

Press any key to sample instrument on port  /dev/ttySX9 :

number of args: 2

SIAM version $Name: march14_2006 $

ASIMET SWR s/n SWR344:

parentID=1446, recordType=1

devid=1292, t=1142567913630, seqNo=439, mdref=438

nBytes=17

    0.6 :   32723

Parser not implemented.
Press any key to get most recent sample from instrument on port  /dev/ttySX9 :

SIAM version $Name: march14_2006 $

parentID=1446, recordType=1

devid=1292, t=1142567913630, seqNo=439, mdref=438

nBytes=17

    0.6 :   32723
Press any key to shutdown service on port  /dev/ttySX9 :

SIAM version $Name: march14_2006 $

Shutdown port /dev/ttySX9

OK

SIAM version $Name: march14_2006 $

Node 1446 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Mooring power can s/n 002            1322    ERROR       0   1   3

/dev/ttySX1  Snubber Node Power Control           1502    OK          1   0   0

/dev/ttySX2  -                                    -       -        -           

/dev/ttySX3  -                                    -       -        -           

/dev/ttySX4  ASIMET BPR s/n BPR222                1443    OK          1   0   0

/dev/ttySX5  MBARI pCO2 s/n SOON1S                1448    ERROR       0   1   0

/dev/ttySX6  Triaxys s/n TAS01020                 1286    SLEEPING    0   0   0

/dev/ttySX7  ASIMET HRH s/n HRH355                1290    OK          1   0   0

/dev/ttySX8  ASIMET WND s/n WND358                1291    OK          1   0   0

/dev/ttySX9  -                                    -       -        -           

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 -                                    -       -        -           

/dev/ttySA2  -                                    -       -        -           

Should now be no service on port  /dev/ttySX9
Press any key to load service on port  /dev/ttySX9 :

SIAM version $Name: march14_2006 $

Scan port /dev/ttySX9

SIAM version $Name: march14_2006 $

Node 1446 has 14 ports

Port name    Service                              ISI-ID  Status    S  : E : R 

---------    -------                              ------  ------   ----------- 

/dev/ttySX0  Mooring power can s/n 002            1322    ERROR       0   1   3

/dev/ttySX1  Snubber Node Power Control           1502    OK          1   0   0

/dev/ttySX2  -                                    -       -        -           

/dev/ttySX3  -                                    -       -        -           

/dev/ttySX4  ASIMET BPR s/n BPR222                1443    OK          1   0   0

/dev/ttySX5  MBARI pCO2 s/n SOON1S                1448    ERROR       0   1   0

/dev/ttySX6  Triaxys s/n TAS01020                 1286    SLEEPING    0   0   0

/dev/ttySX7  ASIMET HRH s/n HRH355                1290    OK          1   0   0

/dev/ttySX8  ASIMET WND s/n WND358                1291    OK          1   0   0

/dev/ttySX9  ASIMET SWR s/n SWR344                1292    OK          1   0   0

/dev/ttySX10 -                                    -       -        -           

/dev/ttySX11 -                                    -       -        -           

/dev/ttySX15 -                                    -       -        -           

/dev/ttySA2  -                                    -       -        -           

Should now be service running on port  /dev/ttySX9
Press any key to get instrument metadata from port  /dev/ttySX9 :

Looking for node server stub at rmi://surface/node

Got proxy for node service "moos.deployed.NodeService"

Requesting packet...components = 0x1f

Packet received:

parentID=1446, recordType=0

devid=1292, t=1142568018442, seqNo=0, mdref=0

 cause=just checking

<DEV_MD>

Requesting cal constants - OK

SWR01
SWR344
VOSSWR53 v3.3
2.4576 Mhz
15AUG05
2006/03/17  04:03:40
SWR: -3.98472e+03  1.21790e-01  0.00000e+00  0.00000e+00
No PCMCIA card installed

MODADR: SWR01
MODMFG: STAR ENG
MODMOD: VOSSWR
MODSER: SWR344
MODDAT: 24OCT03
SENMFG: EPPLEY
SENMOD: PSP
SENSER: 33677F3
SENDAT: 27FEB03
SFTMFG: WHOI/GEOFF
SFTNAM: VOSSWR53
SFTREV: 3.3
SFTDAT: 26NOV03
CALFAC: WHOI
CALPER: J.C.SMITH
CALDAT: 15AUG05
DATFRM: -
DATDES: -
DATUNI: -
RAWFRM: -
RAWDES: -
RAWUNI: -

</DEV_MD>

<SRVC_MD>

moduleAddress=01

powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.asimet.WhoiAsimet$Attributes

serviceName=ASIMET SWR s/n SWR344

parentID=1446

currentLimitMa=2000

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

extendedVersion=UNK

frameworkVersion=$Name: march14_2006 $

UUID=FC5BD33E-E7D6-4CF8-9A17-944A175A2B39

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=3

isiID=1292

sampleTimeoutMsec=3000

commPowerPolicy=SAMPLING

serviceStatus=0

startDelayMsec=4000

sensorType=SWR

</SRVC_MD>

<DOC_MD>

unable to access XML file

</DOC_MD>

Press any key to show schedule for instrument on  /dev/ttySX9 :

ShowSchedule: lookAhead value undefined or invalid; using default (3600)

Looking for node service at rmi://surface/node

Got proxy for node service "moos.deployed.NodeService"

    Name: Default

   Owner: moos.devices.asimet.WhoiAsimet:1292 key=10

Schedule: R */0 */10 */0 */0 * * * * GMT *

  Status: Waiting
553922

Test complete.

surface:/mnt/hda/siam/atp$ 

