MTM2

SIAM Deployment Procedures

To Bring

USB Dongle

Freewave

Freewave serial/power cable

Power supply

MMC console cable

Notebook

Checklist

Login via shorthaul

· Open hyperterm session to freewave (38400N81)

· When Freewave connects (can take up to 5 minutes) login ops:brynner (have 30 seconds)

· Immediately do ‘export TMOUT=0’ to keep console session open

· Remember to use exit before leaving hyperterm

Sample Strain Gauge

· From ops login do gosiam

· Turn on Hyperterm capture file

· Run sampleStrainGauge

· Updates every 10 min.

· ^C stops sampleStrainGauge

Upload P2 and Powercan persistor data

· from ops login do gosiam

· listPorts localhost 0

· shutdownPort localhost 0

· listPorts localhost 0

· powerUpPort localhost 0

· stip –s 38400 /dev/ttySX0

· CR gives RDY prompt

· Exit gets you to PicoDOS

· C:\cd logs

· C:\logs\dir

· C:\logs\ys 1.001 1.002 …TimeSynchLog etc

· Use hyperterm transfer>>receive file>> Y Modem to get files to local machine

· “~.” Exits PicoDOS

· powerDownPort localhost 0

· scanPort localhost 0

· repeat for P2 on port 2

To transfer files from mtm-1 to local PC use YModem

· mtm-1# sz <files…>

· use Hyperterm>>Transfer>>Receive>>Ymodem

To transfer files from local PC to mtm-1 use ZModem

· mtm-1# rz

· Hyperterm>>Transfer>>Send>>Zmodem

Notes/Cautions:

· Sidearm407=mtm-1

· Minicom doesn’t work w/ ymodem on mooring (thus stip)

· RmiClient/rmiServer scripts on mooring can be run (remote, local, or combined) to debug RMI problems)

· If non-local utility, 

· Pon globalstar (takes a while ~ 1 min, look for ppp)

· Will stay up until app downloads; app will shut it down on you when finished

· Poff globalstar 

