[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating left dpa channel
[TEXTIO.0]->Whew, we got the port identifier for 'com1'!!
[TEXTIO.0]->Whew, no one owned com1
[TEXTIO.0]->Whew, com1 turns out to be a serial port...
[TEXTIO.0]->Finished creating the serial port on com1
[TEXTIO.0]->Finished loading left channel
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaRightChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcRight ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->RightRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RightChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating right dpa channel
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Outbound doing blocking dequeue...
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Inbound blocking on socket read...
vm.0 charadeIO active 
vm.0 heap monitor active
vm.0 heap monitor active
[TEXTIO.0]->Starting 'initializePlatform()'
[TEXTIO.0]->DpaBoard ctor invoked
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaLeftChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcLeft ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->LeftRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->LeftChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating left dpa channel
[TEXTIO.0]->Whew, we got the port identifier for 'com1'!!
[TEXTIO.0]->Whew, no one owned com1
[TEXTIO.0]->Whew, com1 turns out to be a serial port...
[TEXTIO.0]->Finished creating the serial port on com1
[TEXTIO.0]->Finished loading left channel
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaRightChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcRight ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->RightRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RightChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating right dpa channel
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Outbound doing blocking dequeue...
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Inbound blocking on socket read...
[TEXTIO.0]->received: %<%msgType=PollCmd%seqNo=1%len=4%channelNumber=0%>%
[TEXTIO.0]->Inbound blocking on socket read...
[TEXTIO.0]->detected poll cmd
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->got input: o=111
[TEXTIO.0]->got input: n=110
[TEXTIO.0]->got input: e=101
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: s=115
[TEXTIO.0]->got input: a=97
[TEXTIO.0]->got input: m=109
[TEXTIO.0]->got input: p=112
[TEXTIO.0]->got input: l=108
[TEXTIO.0]->got input: e=101
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: 5=53
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->Around the loop 0 time(s).
[TEXTIO.0]->Outbound back from blocking dequeue...

[TEXTIO.0]->  with message: %<%msgType=PolledDataReply%seqNo=1%len=32%channelNumber=0%endOfData=true%subseqNo=0%timestamp=64454%data
=one sample1514%>%
[TEXTIO.0]->Cerealizing PolledDataReply, data.length=15
[TEXTIO.0]->  msgStr.length is 44
[TEXTIO.0]->Just sent the outbound message
[TEXTIO.0]->Outbound doing blocking dequeue...
[load]-> -- aJile Charade load script file
[load]-> -- This file was auto-generated
[load]-> 
[load]-> Halt
[load]-> Reset
[load]-> 
[load]-> 
[load]-> load C:/WINDOWS/Profiles/wbaugh/Mbari/sidekick/JemBuilderOutputFiles/build.jcf
Reading file: c:/windows/profiles/wbaugh/mbari/sidekick/jembuilderoutputfiles/build.jcf
Reading file: C:\WINDOWS\Profiles\wbaugh\Mbari\sidekick\JemBuilderOutputFiles\build.bin
 Configuration: SajeConfiguration
 Runtime: Runtime_cldc Version 3.14
 ucode version: 0x2f
C:\WINDOWS\Profiles\wbaugh\Mbari\sidekick\JemBuilderOutputFiles\build.bin
jemcfg 1.7 February 28, 2002 3:20:20 PM PST executive1 
C:\aJile\Runtime_cldc\ucode\aJ-100_uram.bin
 created on Sat Jan 19 22:02:31 2002 (GMT)
Loaded 245184 bytes
== SYSTEM ===========================
=+ Bin file: C:\WINDOWS\Profiles\wbaugh\Mbari\sidekick\JemBuilderOutputFiles\build.bin
== [jemcfg 1.7 February 28, 2002 3:20:20 PM PST executive1]

-- VM #0 ----------------------------
-- RAM start: 000042f8  end: 0005947f (340.4 KB)
-- ROM start: 00059480  end: 000910c7 (223.1 KB)
-+ Map file: C:\WINDOWS\Profiles\wbaugh\Mbari\sidekick\JemBuilderOutputFiles\JVM0.map

File 'c:/windows/profiles/wbaugh/mbari/sidekick/jembuilderoutputfiles/build.jcf' loaded successfully
[load]-> 
[load]-> -- Run User Defined Startup Macro(stored in f.sod file)
[load]-> @setup
Textio mode       (tx): on
[load]-> 
[load]-> 
[load]-> 
vm.0 charadeIO active 
vm.0 heap monitor active
vm.0 heap monitor active
[TEXTIO.0]->Starting 'initializePlatform()'
[TEXTIO.0]->DpaBoard ctor invoked
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaLeftChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcLeft ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->LeftRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->LeftChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating left dpa channel
[TEXTIO.0]->Whew, we got the port identifier for 'com1'!!
[TEXTIO.0]->Whew, no one owned com1
[TEXTIO.0]->Whew, com1 turns out to be a serial port...
[TEXTIO.0]->Finished creating the serial port on com1
[TEXTIO.0]->Finished loading left channel
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaRightChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcRight ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->RightRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RightChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating right dpa channel
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Outbound doing blocking dequeue...
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Inbound blocking on socket read...
[TEXTIO.0]->received: %<%msgType=PollCmd%seqNo=1%len=4%channelNumber=0%>%
[TEXTIO.0]->Inbound blocking on socket read...
[TEXTIO.0]->detected poll cmd
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->got input: m=109
[TEXTIO.0]->got input: i=105
[TEXTIO.0]->got input: c=99
[TEXTIO.0]->got input: r=114
[TEXTIO.0]->got input: o=111
[TEXTIO.0]->got input: c=99
[TEXTIO.0]->got input: a=97
[TEXTIO.0]->got input: t=116
[TEXTIO.0]->got input: r=114
[TEXTIO.0]->got input: e=101
[TEXTIO.0]->got input: s=115
[TEXTIO.0]->got input: p=112
[TEXTIO.0]->got input: o=111
[TEXTIO.0]->got input: n=110
[TEXTIO.0]->got input: s=115
[TEXTIO.0]->got input: e=101
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: 5=53
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->Around the loop 0 time(s).
[TEXTIO.0]->Outbound back from blocking dequeue...

[TEXTIO.0]->  with message: %<%msgType=PolledDataReply%seqNo=1%len=38%channelNumber=0%endOfData=true%subseqNo=0%timestamp=70254%data
=microcatresponse1522%>%
[TEXTIO.0]->Cerealizing PolledDataReply, data.length=21
[TEXTIO.0]->  msgStr.length is 50
[TEXTIO.0]->Just sent the outbound message
[TEXTIO.0]->Outbound doing blocking dequeue...
vm.0 charadeIO active 
vm.0 heap monitor active
vm.0 heap monitor active
[TEXTIO.0]->Starting 'initializePlatform()'
[TEXTIO.0]->DpaBoard ctor invoked
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaLeftChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcLeft ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->LeftRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->LeftChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating left dpa channel
[TEXTIO.0]->Whew, we got the port identifier for 'com1'!!
[TEXTIO.0]->Whew, no one owned com1
[TEXTIO.0]->Whew, com1 turns out to be a serial port...
[TEXTIO.0]->Finished creating the serial port on com1
[TEXTIO.0]->Finished loading left channel
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaRightChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcRight ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->RightRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RightChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating right dpa channel
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Outbound doing blocking dequeue...
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Inbound blocking on socket read...
[TEXTIO.0]->received: %<%msgType=PollCmd%seqNo=1%len=4%channelNumber=0%>%
[TEXTIO.0]->Inbound blocking on socket read...
[TEXTIO.0]->detected poll cmd
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->got input: m=109
[TEXTIO.0]->got input: i=105
[TEXTIO.0]->got input: c=99
[TEXTIO.0]->got input: r=114
[TEXTIO.0]->got input: o=111
[TEXTIO.0]->got input: c=99
[TEXTIO.0]->got input: a=97
[TEXTIO.0]->got input: t=116
[TEXTIO.0]->got input: a=97
[TEXTIO.0]->got input: t=116
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: 5=53
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->Around the loop 0 time(s).
[TEXTIO.0]->Outbound back from blocking dequeue...

[TEXTIO.0]->  with message: %<%msgType=PolledDataReply%seqNo=1%len=32%channelNumber=0%endOfData=true%subseqNo=0%timestamp=49444%data
=microcatat1523%>%
[TEXTIO.0]->Cerealizing PolledDataReply, data.length=15
[TEXTIO.0]->  msgStr.length is 44
[TEXTIO.0]->Just sent the outbound message
[TEXTIO.0]->Outbound doing blocking dequeue...
vm.0 charadeIO active 
vm.0 heap monitor active
vm.0 heap monitor active
[TEXTIO.0]->Starting 'initializePlatform()'
[TEXTIO.0]->DpaBoard ctor invoked
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaLeftChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcLeft ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->LeftRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->LeftChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating left dpa channel
[TEXTIO.0]->Whew, we got the port identifier for 'com1'!!
[TEXTIO.0]->Whew, no one owned com1
[TEXTIO.0]->Whew, com1 turns out to be a serial port...
[TEXTIO.0]->Finished creating the serial port on com1
[TEXTIO.0]->Finished loading left channel
[TEXTIO.0]->DpaChannel ctor invoked
[TEXTIO.0]->DpaRightChannel ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Adc ctor invoked
[TEXTIO.0]->AdcRight ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RelayReg ctor invoked
[TEXTIO.0]->RightRelayReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->RightChannelCtrlReg ctor invoked
[TEXTIO.0]->HdwrReg(int[]) ctor invoked
[TEXTIO.0]->Finished creating right dpa channel
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Outbound doing blocking dequeue...
[TEXTIO.0]->OutboundMessage thread starting...
[TEXTIO.0]->Inbound blocking on socket read...
[TEXTIO.0]->received: %<%msgType=PollCmd%seqNo=1%len=4%channelNumber=0%>%
[TEXTIO.0]->Inbound blocking on socket read...
[TEXTIO.0]->detected poll cmd
[TEXTIO.0]->got input: 
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: B=66
[TEXTIO.0]->got input: E=69
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: 7=55
[TEXTIO.0]->got input: -=45
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: M=77
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->got input: T=84
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: .=46
[TEXTIO.0]->got input: 9=57
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: 5=53
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: .=46
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 7=55
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: -=45
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: -=45
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: 9=57
[TEXTIO.0]->got input: 8=56
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: :=58
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: :=58
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->Driver: 'TheMicroCatDriverRev2' got timeout
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->got input: T=84
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: .=46
[TEXTIO.0]->got input: 9=57
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: 9=57
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: .=46
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 6=54
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: -=45
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: -=45
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: 9=57
[TEXTIO.0]->got input: 8=56
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: :=58
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: 5=53
[TEXTIO.0]->got input: :=58
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->Driver: 'TheMicroCatDriverRev2' got timeout
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->got input: T=84
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: .=46
[TEXTIO.0]->got input: 9=57
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: 8=56
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: .=46
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 6=54
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: -=45
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 3=51
[TEXTIO.0]->got input: -=45
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: 9=57
[TEXTIO.0]->got input: 8=56
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: ,=44
[TEXTIO.0]->got input:  =32
[TEXTIO.0]->got input: 0=48
[TEXTIO.0]->got input: 1=49
[TEXTIO.0]->got input: :=58
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: 5=53
[TEXTIO.0]->got input: :=58
[TEXTIO.0]->got input: 2=50
[TEXTIO.0]->got input: 4=52
[TEXTIO.0]->got input: =13
[TEXTIO.0]->got input: 
[TEXTIO.0]->=10
[TEXTIO.0]->got input: S=83
[TEXTIO.0]->got input: >=62
[TEXTIO.0]->Driver: 'TheMicroCatDriverRev2' got timeout
[TEXTIO.0]->Error during poll, error text=java.lang.Exception: Retry limit exceeded (retries=3)
[TEXTIO.0]->Uncaught Exception
[TEXTIO.0]->   java.lang.NullPointerException
[TEXTIO.0]->no Stack Trace
