Basic FITA Installation Procedures
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Installation Procedure Steps

The installation procedure covers the following generic steps in the assembly and test of the FITA to customer’s cable:-

• Prepare the cables to length.

• Install FITA

• Water Test – Fill Termination with water to verify the integrity of boot seals.

• Helium/Dry Nitrogen Pressure Test – Fill Termination with Helium/Dry Nitrogen and pressurize to verify integrity of housing/compensator assembly.

Environmental Conditions:

Temperature requirements Minimum 65(F Maximum 98(F

Materials Required To Be Supplied By Customer:

· Helium/Dry Nitrogen

· Clean Dry Working Space Approximately 12 feet X 12 feet

· Power Source for electrical equipment 110 or 240 volt single phase

· Work bench

· Vice

· Rags / Paper Towels

· Lighting

· Trap or tent during rainy and hot conditions.

· Compressed air (if available).
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