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WETStar 

Miniature Fluorometer

The WETStar miniature chlorophyll fluorometer is the first of a new class of miniaturized, low cost, low power optical instruments.  WETStar provides comparable performance to other available fluorometers at a fraction of their cost, power and size.  The unit employs a novel flow tube optical design, which lends itself to both pump-through and flow-through operation.  The unit’s 7–15 VDC input power range and 0–5 VDC analog output allow it to easily mate with existing CTD packages.  WETStar is available with a delivery time of four to six weeks.

	Specifications

Mechanical

Length: 6.7 in (17.1 cm)

Diameter: 2.7 in (6.9 cm)

Weight


in air: 1.7 lbs (0.8 kg)

in water: 0.25 lbs (0.1 kg)

Rated Depth: 600 meters

Electrical

Response Time: 0.17 sec

Input Voltage: 7–15 VDC

Output Voltage: 0–5 VDC

Power requirement: <450 mW

Optical

Sensitivity: ≥ 0.03 (g/l

Wavelength excitation: 470 nm

Wavelength emission: 685 nm

Dynamic Range: 0.03–75(g/l

Other ranges on request
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Specifications are subject to change without notice.

WETStar

Specifications Sheet

WET Labs, Inc.

P.O. Box 518

Philomath, OR 97370

Tel: 541-929-5650

fax: 541-929-5277

email: wetlabs@wetlabs.com

http://www.wetlabs.com
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	12/01/99
	Begin revision control
	H. Van Zee

	B
	01/03/00
	Change depth rating; add excitation and emission
	D. Hankins

	C
	12/12/00
	Change sensitivity range
	D. Hankins

	D
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	Revise ex and em values (DCR 164)
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