BIN Final Pre-Dive Checklist
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1.0 Checklist covers the BIN mooring controller, power system "ready-to-be launched" final shipboard readiness level.

	Deployment
	25 April 2007 Shelf Swap

	Test date
	25 April

	Node Application
	Shelf backup

	Node Name
	Naviti


2.0 Final Checklist.
2.1 Verify housing internal pressure and humidity readings.

2.1.1 □ Pressure between 800-900 mB. Reading

2.1.2 □ Humidity < 25%. Reading 

2.2 □ Loopback the electro/optical ROVMate plug connector using either loopback test receptacle or a lab jumper and verify and record loopback optical power levels at each Medusa port pair using the Medusa ‘loopback’ command. Received power must be greater than -15dB with full deployed hardware including Benthic cable or -10dB with just loopback connector.

	
	Loopback 0-1
	Loopback 2-3
	Test conditions

	Port REC PWR dB
	0 =
	2 =
	

	Port REC PWR dB
	1 = 
	3 =
	


2.3 □ Check backup battery voltage. SamplePort loc /dev/ttySX13 Voltage on ADC 13 must be greater than 12.5 VDC. Record reading:
2.4 □ Perform final check that all cables are securely tie-wrapped in place.
2.5 □ Verify HomerPro beacon with fresh batteries is installed and record beacon number.
2.6 Remove protective caps on all instruments:
2.6.1 □ Aquadopp

2.6.2 □ O2 sensor

2.6.3 □ SBE 16 CTD
2.6.4 □ ADCP (Teledyne/RDI)
2.6.5 □ WetLabs
2.7 Verify elevator RF beacon and optical strobe are turned on.



2.7.1 □ RF beacon.  VHF channel 
2.7.2 □ Optical strobe.






