[image: image1.jpg]1, Center strength member, daouble
braided nylon or polyester rope,
1.0” 0.D.

2, Jacket over CSM (PU or Hytrel
0.03” to 006" thickness, 106" OD

3, Conductors, Hi-Wire #18 AGW
construction, 8 units, 0147 0.D.

4, Optical fiber bend sensors with
Jacketing, 4 units,
014" thickness, 134" 0D

S, Extruded jocket, to enclose
conductors, Hytrel, 1.28” O.D

6, Outer bedding braid, Polyester,
011 thickness, total coble 0D, 1.5




