
MOOS mooring telemetry is received via PC running the SIAM portal application. The mooring
initiates contact by establishing a PPP link with the portal, creating a socket and writing a message to the socket, indicating that it is available. In general, the portal implements logic to decide what, if any, operations are to be performed in the connection session

Four plots used to characterize MOOS mooring telemetry are described below:

portalProfile

opTimeDistribution

bitrateVsTransferSize

packetSizeVsDeviceID