Float/Cable Tank Test 3/18/03

Single Float Test:


A single float was place on a piece of cable and stretched between two points as shown in the diagram.  The three photos show the configuration of the float and cable at a cable tension of 10 lbs, 40 lbs, and 60 lbs.
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a) Schematic               



  b) Tension = 10 lbs
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  c) Tension = 40 lbs



  d) Tension = 60 lbs

Double Float Test:


Two floats were placed on a piece of cable and stretched between two points as shown.  A 15 lb weight (representing 50 meters of cable in water) was placed between the two floats. 
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50lb Tension
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100lb Tension
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150lb Tension
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200lb Tension
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