MOOS Mooring 11/29/06 Meeting Agenda

1) Project current status, budget and resources.

2) Status of MSE datastreams:

	MSE Surface Node - June 2006 · log

	    Instrument
	Data
	Plots

	      Radiometer-Shortwave - ended 2006-10-27T18:48:31Z 
        ASIMET SWR - 1557
	DataStream · netCDF · log 
	full deployment 

	      Environment Monitor-System 
        MSP430 - 1447
	DataStream 
	 

	      Cable Monitor (??)
        Snubber Node Power Control (P2) - 1502
	 
	 

	      Meteorology Package - ended 2006-10-27T18:39:16Z 
        ASIMET HRH - 1290
	DataStream · netCDF · log 
	full deployment 

	      Wind Sensor  *DEAD, NEEDS REPLACING
        ASIMET WND - 1291
	DataStream · netCDF · log 
	full deployment 

	      Air Pressure Sensor 
        ASIMET BPR - 1443
	DataStream 
	 

	      ADCP - ended 2006-10-27T18:51:36Z 
        Workhorse Long Ranger 75KHz ADCP - 1294
	DataStream · log 
	full deployment 

	      CO2 Monitor 
        SOON/PCO2 - 1448
	DataStream 
	 

	      Wave Sensor  *DEAD, NEEDS REPLACING
        Triaxys Directional Wave Sensor - 1286
	 
	 

	      Meteorology Package *DEAD, NEEDS REPLACING
        ASIMET HRH - 1290
	DataStream · netCDF · log 
	full deployment | last 7 days 

	      Radiometer-Shortwave 
        ASIMET SWR - 1557
	DataStream · netCDF · log 
	full deployment | last 7 days 

	      ADCP

      Workhorse Long Ranger 75KHz ADCP - 1294
	DataStream · log 
	full deployment | last 7 days 

	      GPS 
        GPS - 1566
	 
	 

	
	DataStream · netCDF · log 
	full deployment | last 7 days


	MSE Secondary Surface Node - June 2006 · log

	    Instrument
	Data
	Plots

	      Radiometer-Longwave - ended 2006-10-27T16:38:10Z 
        ASIMET LWR - 1289
	DataStream · netCDF · log 
	full deployment 

	      CTD @ 1.0 m - ended 2006-10-27T16:50:53Z 
        CTD - 1277
	DataStream · netCDF · log 
	full deployment 

	      Radiometer-Hyperspectral *CIMT-LIKE PLOTS?
        HyperOCR-I - 1517
	DataStream 
	 

	      CTD 
        CTD - 1277
	DataStream · netCDF · log 
	full deployment | last 7 days 

	      Nitrogen Sensor-ISUS 
        Satlantic ISUS - 1514
	DataStream 
	 

	      GPS 
        GPS - 1504
	 
	 

	
	DataStream · netCDF · log 
	full deployment | last 7 days 

	      Radiometer-Longwave 
        ASIMET LWR - 1289
	DataStream · netCDF · log 
	full deployment | last 7 days 

	      Fluorometer 
        Combination Turbidity and Fluorescence Sensor – 1530 *DATA IS SAME AS SHELF AND AXIS INSTRUMNENTS (WITHOUT SUMMARY) CAN BE PLOTTED??
	DataStream 
	 

	      Oxygen Sensor Y axis should be labeled "mmol per liter" as shown in the sensor meta-data
        Aanderaa Oxygen Optode – 1460 *NOT RETURNING DATA
	 
	 


Data returned: ERR: :readUntil() Timed out:readUntil() Timed out:readUntil() Timed out:retry limit exceeded (3):port OK (1x since 1164630876 s
	MSE 20m Snubber Node - June 2006 · log

	    Instrument
	Data
	Plots

	      Radiometer-Hyperspectral*CIMT-LIKE PLOTS? 
        Satlantic HyperOCR - 1516
	DataStream 
	 

	      CTD @ 20.0 m 
        Seabird 37SMP - 1508
	DataStream · netCDF · log 
	full deployment | last 7 days 

	      Radiometer-Hyperspectral *CIMT-LIKE PLOTS?
        Satlantic HyperOCR - 1515
	DataStream 
	 


	MSE Shelf BIN Node - July 2006 · log

	    Instrument
	Data
	Plots

	      Backscatterometer 
        WETLabs Triplet - 1535
	Summary DataStream · netCDF · log 
	full deployment | last 7 days 

	
	 
	 

	      Currents Sensor-ADCP *Broken summarizer??
        Aquadopp Current Meter - 1474
	Summary DataStream · netCDF · log 
	full deployment 

	
	DataStream 
	 

	      Oxygen Sensor Y axis should be labeled "mmol per liter" as shown in the sensor meta-data
        Aanderaa Oxygen Optode - 1444
	 
	 

	
	Summary DataStream · netCDF · log 
	full deployment | last 7 days 

	      CTD 
        Seabird SBE-16+ - 1533
	 
	 

	
	Summary DataStream · log 
	full deployment | last 7 days 

	      Currents Sensor-ADCP 
        Workhorse ADCP - 1525
	Summary DataStream · netCDF · log 
	full deployment | last 7 days 

	
	 
	 


	MSE Axis BIN Node - November 2006 · log

	    Instrument
	Data
	Plots

	      Currents Sensor-ADCP *Should be in Earth?
        Workhorse Sentinal 300KHz ADCP - 1549
	 
	 

	
	Summary DataStream · netCDF · log 
	full deployment 

	      Optical *NO DATA, NO PLOT
        Combination Turbidity and Fluorescence Sensor - 1537
	 
	 

	      Oxygen *NO PLOT SHOWN 
        Aanderraa Oxygen Optode - 1445
	 
	 

	
	Summary DataStream 
	 

	      ADCP 
        Aquadopp Current Meter - 1473
	Summary DataStream · netCDF · log 
	full deployment | last 7 days 

	
	 
	 

	      CTD - ended 2006-11-20T22:34:24Z 
        SBE16+ CTD – 1546 *JUMP IN V-0 READING
	Summary DataStream · netCDF · log 
	full deployment | last 7 days 

	
	 
	 

	      CTD *WHY NEW DATA RECORD?
        SBE16+ CTD - 1546
	 
	 

	
	Summary DataStream · netCDF · log 
	full deployment | last 7 days


3) Data telemetry delays and dropped data.

From SIAM notes:

“Analyze MSE telemetry backlogs

11/27: Chaffey believes that retrieval efficiency decreases with stream backlog. 
11/28: As experiment, reversed order of subnode telem retrieval by portal - will axis stay caught up? Also consider: a) feed all node WDTs before telem retrieval b) Look at TCP/IP timeout property settings - may be spending too much time on unresponsive node c) use very long lease for each packet set. Appears to be "stuck" on axis Aquadopp - no telemetry for subsequent data streams, LOTS of Aquadopp error msgs - Try shutting down Aquadopp service? Headley working on profiler, will check in.”
4) Other problems to watch:


A) AXIS GF:





 
SHELF GF:





B) 400V GF. 




C) SNUBBER HUMIDITY.





C) SURFACE PRESSURE (HUMIDITY OK).



 



D) SURFACE GF’s.







