Seabird SBE 37SM (ID 1534) - AXIS
1. Commands issued to instrument by service at initialization 

"STOP" 
(Stop autonomous logging by instrument - If was in safeMode).

"TSS"  
(Take sample, log to instrument's FLASH if service property LOG 

            
set to True (default) , else)

"TS"   
(Take sample, do NOT log to instrument's FLASH)

"MMDDYY=" 

"HHMMSS=" (Sets instrument clock to RTC now)

2. Commands issued by service for safe mode, if applicable
"MMDDYY=" 

"HHMMSS=" (Sets instrument clock to RTC now)

"INTERVAL=" (Set sample interval (seconds). Default is 300s.)

"STARTNOW" (Start autonomous sampling immediately.)

3. Device metadata returned in SIAM datastream
"DS" (Get Status Info)
SBE37-SM-PUCK V 1.0-01  SERIAL NO. 2765    20 Oct 2006  16:02:25

logging not started

sample interval = 60 seconds

samplenumber = 4759, free = 178443

do not transmit real-time data

do not output salinity with each sample

do not output sound velocity with each sample

store time with each sample

number of samples to average = 4

serial sync mode disabled

wait time after serial sync sampling = 30 seconds

PUCK mode enabled

internal pump not installed

temperature = 21.66 deg C

SBE37-SM-PUCK V 1.0-01  2765

temperature:  12-dec-02

    -4.215792e-05

    2.839508e-04

    -3.000133e-06

    1.696669e-07

conductivity:  12-dec-02

    -1.051158e+00

    1.466496e-01

    -9.150801e-05

    3.157882e-05

    -9.570000e-08

    3.250000e-06

    0.000000e+00

pressure S/N 2598, range = 160 psia:  09-dec-02

    5.945600e-02

    7.603297e-03

    -7.831820e-10

    5.468956e+01

    1.021594e+00

    -2.910683e-02

    2.494063e+01

    9.250000e-04

    0.000000e+00

    0.000000e+00

rtc:  12-dec-02

    9.999726e-01

    1.708880e-06

    -3.062022e-08

4. Instrument-specific service properties
/** Log to instrument’s FLASH. Default is true. */

log = true;
/** Set Safe Sample Interval in Seconds */

safeSampleIntervalSec = 300;    //Default to 5 minutes.

5. Initial service property values for this deployment
powerOnDelaySec=0

nominalCurrentMa=1000

summaryVars=temperature conductivity Pressure Voltage-0 Voltage-1 

serviceName=Seabird-37SM s/n 37SM30960-2765

packetSetSize=10

sampleSchedule=R */10 */0 */0 */0 * * * * GMT *

defaultSkipInterval=0

UUID=a7c7f011-b481-11da-a94d-0800200c9a66

timeSynch=false

maxSampleTries=3

isiID=1534

log=true

peakCurrentMa=5000

sampleTimeoutMsec=15000

safeSampleIntervalSec=300

serviceStatus=5

startDelayMsec=2000

isiID = 1534

sampleSchedule = 10

powerPolicy = always

commPowerPolicy = sampling

currentLimitMa=3000

summaryTriggerCount = 360

maxSummarySamples = 360

6. Results of acceptance test procedures
All OK.

7. Summarization

Summarization working?   Yes.

Sampling Once every hour (10 x 360 = 3600)

sampleSchedule = 10

summaryTriggerCount = 360

maxSummarySamples = 360
8. Instrument clock synchronization

Sets to RTC.     setClock(System.currentTimeMillis());
9. Known-service bugs/deficiencies

Does not consistently go into “safe” mode 






