BIN 400-12V Switch (ID 1593)
1. Commands issued to instrument by service at initialization 

”APP\r” – verify that application is running
binBackups(false,true) – Disable backup batt, enable caps
2. Commands issued by service for safe mode, if applicable
NONE
3. Device metadata returned in SIAM datastream
parentID=1522, recordType=0

devid=1593, t=1161721515787, seqNo=0, mdref=0

 cause=just checking

<SRVC_MD>

powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.serialadc.SerialAdc$Attributes

captureParams=ADC BP

serviceName=BIN 400-12V Switch s/n 1.04

parentID=1522

maxSummarySamples=0

currentLimitMa=3000

packetSetSize=10

enableBackupCapacitors=true

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

enableBackupBatteries=false

defaultSkipInterval=0

statusMinSamples=10

extendedVersion=UNK

frameworkVersion=$Name: october20_2006-2 $

errCacheLimit=5

UUID=3e9307c0-5ee0-11db-9a46-713f51a86ba0

powerWarningLow=11.0

powerPolicy=NEVER

timeSynch=false

powerOkLow=12.0

maxSampleTries=3

isiID=1593

powerStatusChannel=ADC10

peakCurrentMa=5000

summaryTriggerCount=0

dataCountCheck=true

sampleTimeoutMsec=5000

commPowerPolicy=SAMPLING

serviceStatus=0

logTimeSync=true

startDelayMsec=10000

</SRVC_MD>

<SVP_MD>

isiID = 1593

serviceName = BIN 400-12V Switch s/n 1.04

powerPolicy = never

commPowerPolicy = sampling

sampleSchedule = 600

captureParams = ADC BP

dataCountCheck = true

logTimeSync = true

powerStatusChannel = ADC10

powerWarningLow=11.0

powerOkLow=12.0

statusMinSamples = 10

currentLimitMa = 3000

sampleTimeoutMsec=15000

UUID = 3e9307c0-5ee0-11db-9a46-713f51a86ba0

</SVP_MD>

<DEV_MD>

VERSION:

MOOS POWER SYSTEM DAQ 0.7

built on May  9 2006 at 21:57:13

CVS tag "$Name:  $"

CONFIGURATION:

ADC00 S09 C01 P0001000 T0000000 D0 L0 A1

ADC01 S09 C02 P0000250 T0000000 D0 L0 A1

ADC02 S09 C03 P0000250 T0000000 D0 L0 A1

ADC03 S09 C04 P0000250 T0000000 D0 L0 A1

ADC04 S09 C05 P0000250 T0000000 D0 L0 A1

ADC05 S09 C06 P0000250 T0000000 D0 L0 A1

ADC10 S10 C01 P0001000 T0000000 D0 L0 A1

ADC11 S10 C02 P0000250 T0000000 D0 L0 A1

ADC12 S10 C03 P0001000 T0000000 D0 L0 A1

ADC13 S10 C04 P0001000 T0000000 D0 L0 A1

ADC14 S10 C05 P0001000 T0000000 D0 L0 A1

DO00 S-1 C-1 E0000000 D0000000  O0 A1

BP00 S09 C07 P0000250 A1

CALIBRATION:

S09 C01 G+1.5157e-02 O+0.0000e+00

S09 C02 G+7.3240e-06 O+0.0000e+00

S09 C03 G+7.3240e-06 O+0.0000e+00

S09 C04 G+1.1100e-05 O+0.0000e+00

S09 C05 G+1.1100e-05 O+0.0000e+00

S09 C06 G+1.1100e-05 O+0.0000e+00

S10 C01 G+5.6400e-04 O+0.0000e+00

S10 C02 G+4.5780e-04 O+0.0000e+00

S10 C03 G+5.6400e-04 O+0.0000e+00

S10 C04 G+5.6400e-04 O+0.0000e+00

S10 C05 G+2.0220e-01 O-2.7315e+02

CALIBRATION REV "$Revision: 1.13 $"
4. Instrument-specific service properties
 /** _dataCountCheck can be enabled and disabled via property */

boolean dataCountCheck = false;

/** _logTimeSync can be enabled and disabled via property */

boolean logTimeSync = false;

/** Default DATA CAPTURE and DATA FETCH parameters */

String captureParams = "ALL\r";

/** String to parse for to find powerStatusFlag */

String powerStatusChannel="ADC99";

/** Power OK lower threshold (should be > powerWarningLow) */

double powerOkLow=0;

/** Power WARNING lower threshold (should be > 0) */

double powerWarningLow=0;

/** Minimum samples for to validate power status */

int statusMinSamples=20;

/** Set state of backup batteries at service start  */

boolean enableBackupBatteries = false;

/** Set state of backup caps at service start  */

boolean enableBackupCapacitors = true;
5. Initial service property values for this deployment
powerPolicy=NEVER
commPowerPolicy=SAMPLING

sampleSchedule=600

captureParams= ADC BP

dataCountCheck=true

logTimeSynch=true
powerStatusChannel= ADC10

powerWarningLow=11.0

powerOkLow=12.0

statusMinSamples=10

currentLimitMa=3000

sampleTimeoutMsec=15000

UUID= 3e9307c0-5ee0-11db-9a46-713f51a86ba0
6. Results of acceptance test procedures
PASS
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7. Summarization

NONE
8. Known-service bugs/deficiencies

NONE






_1223203145/POWER_ATP_AXIS_Pass.TXT
node=//loc/node
port=/dev/ttySX13
SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
958 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
959 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
2720 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
2722 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Node 1522 has 14 ports

Port name    ISI-ID  Service                              Status    S  : E : R 
---------    ------  -------                              ------   ----------- 
3778 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
3779 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
/dev/ttySX13 1593    BIN 400-12V Switch s/n 1.04          OK          1   0   0
/dev/ttySX1  -       -                                    -        -           
/dev/ttySX2  -       -                                    -        -           
/dev/ttySX3  -       -                                    -        -           
/dev/ttySX4  -       -                                    -        -           
/dev/ttySX5  -       -                                    -        -           
/dev/ttySX6  -       -                                    -        -           
/dev/ttySX7  -       -                                    -        -           
/dev/ttySX8  -       -                                    -        -           
/dev/ttySX9  -       -                                    -        -           
/dev/ttySX10 -       -                                    -        -           
/dev/ttySX11 -       -                                    -        -           
/dev/ttySX15 -       -                                    -        -           
/dev/ttySA2  -       -                                    -        -           

1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
Looking for node server stub at rmi://loc/node
685 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
687 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
1789 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1791 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Got proxy for node service "moos.deployed.NodeService"
2478 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
2479 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Press any key to sample instrument on port  /dev/ttySX13 :number of args: 2
SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
908 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
910 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
4512 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
4513 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
5472 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
5473 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
BIN 400-12V Switch s/n 1.04:
parentID=1522, recordType=1
devid=1593, t=1161721317825, seqNo=575, mdref=574
nBytes=719
ADC00 A+3.0651e-01 N0000072 L+3.0314e-01 H+3.1830e-01 E0

ADC01 A-3.2409e-06 N0000287 L-1.4648e-05 H+7.3240e-06 E0

ADC02 A-2.1436e-06 N0000287 L-7.3240e-06 H+7.3240e-06 E0

ADC03 A-5.3760e-06 N0000287 L-2.2200e-05 H+1.1100e-05 E0

ADC04 A-2.9007e-06 N0000287 L-1.1100e-05 H+1.1100e-05 E0

ADC05 A-2.4753e-06 N0000287 L-2.2200e-05 H+1.1100e-05 E0

ADC10 A+1.2735e+01 N0000072 L+1.2339e+01 H+1.3117e+01 E0

ADC11 A-5.4961e-01 N0000287 L-6.5511e-01 H-4.8618e-01 E0

ADC12 A+1.2816e+01 N0000072 L+1.2419e+01 H+1.3200e+01 E0

ADC13 A+4.6420e-02 N0000072 L+4.3428e-02 H+5.4708e-02 E0

ADC14 A+2.6516e+01 N0000072 L+2.6510e+01 H+2.6713e+01 E0

BP00 N0000287 A0287 B0287 C0000 D0287 E0000 F0287 G0000 H0000

DATA COUNT 00701


Press any key to get most recent sample from instrument on port  /dev/ttySX13 :SIAM version $Name: october20_2006-2 $
0 [main] DEBUG moos.operations.utils.NodeUtility  - getNodeURL(): input=//loc/node
0 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
760 [main] DEBUG moos.utils.SiamSocketFactory  - SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
760 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
763 [main] DEBUG moos.utils.SiamSocketFactory  - return new Socket(host, port)...
763 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
1799 [main] DEBUG moos.utils.SiamSocketFactory  - SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1799 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1802 [main] DEBUG moos.utils.SiamSocketFactory  - return new Socket(host, port)...
1802 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
2377 [main] DEBUG moos.utils.SiamSocketFactory  - SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
2377 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
2379 [main] DEBUG moos.utils.SiamSocketFactory  - return new Socket(host, port)...
2379 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
parentID=1522, recordType=1
devid=1593, t=1161721317825, seqNo=575, mdref=574
nBytes=719
ADC00 A+3.0651e-01 N0000072 L+3.0314e-01 H+3.1830e-01 E0

ADC01 A-3.2409e-06 N0000287 L-1.4648e-05 H+7.3240e-06 E0

ADC02 A-2.1436e-06 N0000287 L-7.3240e-06 H+7.3240e-06 E0

ADC03 A-5.3760e-06 N0000287 L-2.2200e-05 H+1.1100e-05 E0

ADC04 A-2.9007e-06 N0000287 L-1.1100e-05 H+1.1100e-05 E0

ADC05 A-2.4753e-06 N0000287 L-2.2200e-05 H+1.1100e-05 E0

ADC10 A+1.2735e+01 N0000072 L+1.2339e+01 H+1.3117e+01 E0

ADC11 A-5.4961e-01 N0000287 L-6.5511e-01 H-4.8618e-01 E0

ADC12 A+1.2816e+01 N0000072 L+1.2419e+01 H+1.3200e+01 E0

ADC13 A+4.6420e-02 N0000072 L+4.3428e-02 H+5.4708e-02 E0

ADC14 A+2.6516e+01 N0000072 L+2.6510e+01 H+2.6713e+01 E0

BP00 N0000287 A0287 B0287 C0000 D0287 E0000 F0287 G0000 H0000

DATA COUNT 00701


Press any key to suspend service on port  /dev/ttySX13 :SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
614 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
615 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
1648 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1649 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
673 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
674 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
1748 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1749 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Node 1522 has 14 ports

Port name    ISI-ID  Service                              Status    S  : E : R 
---------    ------  -------                              ------   ----------- 
3299 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
3301 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
/dev/ttySX13 1593    BIN 400-12V Switch s/n 1.04          SUSPEND     2   0   0
/dev/ttySX1  1534    Seabird-37SM s/n 37SM30960-2765      SAMPLING    5   0   1
/dev/ttySX2  1537    WETLabs ECO-Triplet s/n WL-30011     OK          3   0   0
/dev/ttySX3  -       -                                    -        -           
/dev/ttySX4  -       -                                    -        -           
/dev/ttySX5  -       -                                    -        -           
/dev/ttySX6  -       -                                    -        -           
/dev/ttySX7  -       -                                    -        -           
/dev/ttySX8  -       -                                    -        -           
/dev/ttySX9  -       -                                    -        -           
/dev/ttySX10 -       -                                    -        -           
/dev/ttySX11 -       -                                    -        -           
/dev/ttySX15 -       -                                    -        -           
/dev/ttySA2  -       -                                    -        -           

Service hould now be SUSPENDED on port  /dev/ttySX13
Press any key to resume service on port  /dev/ttySX13 :SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
953 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
954 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
2277 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
2279 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
684 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
685 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
1662 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1663 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Node 1522 has 14 ports

Port name    ISI-ID  Service                              Status    S  : E : R 
---------    ------  -------                              ------   ----------- 
2578 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
2579 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
/dev/ttySX13 1593    BIN 400-12V Switch s/n 1.04          OK          2   0   0
/dev/ttySX1  1534    Seabird-37SM s/n 37SM30960-2765      SAMPLING    7   0   1
/dev/ttySX2  1537    WETLabs ECO-Triplet s/n WL-30011     OK          5   0   0
/dev/ttySX3  1473    Aquadopp Current Meter s/n AQD1997   INIT        0   0   0
/dev/ttySX4  -       -                                    -        -           
/dev/ttySX5  -       -                                    -        -           
/dev/ttySX6  -       -                                    -        -           
/dev/ttySX7  -       -                                    -        -           
/dev/ttySX8  -       -                                    -        -           
/dev/ttySX9  -       -                                    -        -           
/dev/ttySX10 -       -                                    -        -           
/dev/ttySX11 -       -                                    -        -           
/dev/ttySX15 -       -                                    -        -           
/dev/ttySA2  -       -                                    -        -           

Service hould now be OK/SAMPLING on port  /dev/ttySX13
Press any key to shutdown service on port  /dev/ttySX13 :SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
965 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
968 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
1910 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1939 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Shutdown port /dev/ttySX13
OK
SIAM version $Name: october20_2006-2 $
0 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
1230 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
1232 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
3127 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
3128 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Node 1522 has 14 ports

Port name    ISI-ID  Service                              Status    S  : E : R 
---------    ------  -------                              ------   ----------- 
/dev/ttySX13 -       -                                    -        -           
4596 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
4597 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
/dev/ttySX1  1534    Seabird-37SM s/n 37SM30960-2765      SAMPLING   10   0   1
/dev/ttySX2  1537    WETLabs ECO-Triplet s/n WL-30011     OK          8   0   0
/dev/ttySX3  1473    Aquadopp Current Meter s/n AQD1997   OK          2   0   0
6666 ERROR  PortLister [main]: Unexpected DeviceNotFound:
org.mbari.isi.interfaces.DeviceNotFound: 0 not found


Stack trace:


/dev/ttySX4  0                                            
/dev/ttySX5  -       -                                    -        -           
/dev/ttySX6  -       -                                    -        -           
/dev/ttySX7  -       -                                    -        -           
/dev/ttySX8  -       -                                    -        -           
/dev/ttySX9  -       -                                    -        -           
/dev/ttySX10 -       -                                    -        -           
/dev/ttySX11 -       -                                    -        -           
/dev/ttySX15 -       -                                    -        -           
/dev/ttySA2  -       -                                    -        -           

Should now be no service on port  /dev/ttySX13
Press any key to load service on port  /dev/ttySX13 :SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
963 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
965 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
3277 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
3278 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Scan port /dev/ttySX13
33287 DEBUG  SiamSocketFactory [RMI-Leaser]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
33287 DEBUG  SiamSocketFactory [RMI-Leaser]: return new Socket(host, port)...
SIAM version $Name: october20_2006-2 $
1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
1087 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
1088 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
2438 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
2439 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Node 1522 has 14 ports

Port name    ISI-ID  Service                              Status    S  : E : R 
---------    ------  -------                              ------   ----------- 
3598 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
3599 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
/dev/ttySX13 1593    BIN 400-12V Switch s/n 1.04          OK          1   0   0
/dev/ttySX1  1534    Seabird-37SM s/n 37SM30960-2765      SAMPLING   17   0   1
/dev/ttySX2  1537    WETLabs ECO-Triplet s/n WL-30011     SAMPLING   15   0   0
/dev/ttySX3  1473    Aquadopp Current Meter s/n AQD1997   SAMPLING   31   0   0
/dev/ttySX4  1445    Aanderaa Optode s/n 605              OK          7   0   0
/dev/ttySX5  1510    McLane Profiler s/n 001              SAMPLING    0   0   0
/dev/ttySX6  -       -                                    -        -           
/dev/ttySX7  1549    WH Sentinel ADCP 300kHz s/n 2025     SLEEPING    0   0   0
/dev/ttySX8  -       -                                    -        -           
/dev/ttySX9  -       -                                    -        -           
/dev/ttySX10 -       -                                    -        -           
/dev/ttySX11 -       -                                    -        -           
/dev/ttySX15 -       -                                    -        -           
/dev/ttySA2  -       -                                    -        -           

Should now be service running on port  /dev/ttySX13
Press any key to get instrument metadata from port  /dev/ttySX13 :1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
Looking for node server stub at rmi://loc/node
732 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
733 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
3227 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
3229 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Got proxy for node service "moos.deployed.NodeService"
3946 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
3948 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Requesting packet...components = 0x1f
Packet received:

parentID=1522, recordType=0
devid=1593, t=1161721515787, seqNo=0, mdref=0
 cause=just checking
<SRVC_MD>
powerOnDelaySec=0
instrumentName=UNKNOWN
nominalCurrentMa=1000
className=moos.devices.serialadc.SerialAdc$Attributes
captureParams=ADC BP

serviceName=BIN 400-12V Switch s/n 1.04
parentID=1522
maxSummarySamples=0
currentLimitMa=3000
packetSetSize=10
enableBackupCapacitors=true
sampleSchedule=R */0 */10 */0 */0 * * * * GMT *
enableBackupBatteries=false
defaultSkipInterval=0
statusMinSamples=10
extendedVersion=UNK
frameworkVersion=$Name: october20_2006-2 $
errCacheLimit=5
UUID=3e9307c0-5ee0-11db-9a46-713f51a86ba0
powerWarningLow=11.0
powerPolicy=NEVER
timeSynch=false
powerOkLow=12.0
maxSampleTries=3
isiID=1593
powerStatusChannel=ADC10
peakCurrentMa=5000
summaryTriggerCount=0
dataCountCheck=true
sampleTimeoutMsec=5000
commPowerPolicy=SAMPLING
serviceStatus=0
logTimeSync=true
startDelayMsec=10000
</SRVC_MD>
<SVP_MD>
isiID = 1593
serviceName = BIN 400-12V Switch s/n 1.04
powerPolicy = never
commPowerPolicy = sampling
sampleSchedule = 600
captureParams = ADC BP
dataCountCheck = true
logTimeSync = true
powerStatusChannel = ADC10
powerWarningLow=11.0
powerOkLow=12.0
statusMinSamples = 10
currentLimitMa = 3000
sampleTimeoutMsec=15000
UUID = 3e9307c0-5ee0-11db-9a46-713f51a86ba0
</SVP_MD>
<DEV_MD>
VERSION:

MOOS POWER SYSTEM DAQ 0.7

built on May  9 2006 at 21:57:13

CVS tag "$Name:  $"

CONFIGURATION:

ADC00 S09 C01 P0001000 T0000000 D0 L0 A1

ADC01 S09 C02 P0000250 T0000000 D0 L0 A1

ADC02 S09 C03 P0000250 T0000000 D0 L0 A1

ADC03 S09 C04 P0000250 T0000000 D0 L0 A1

ADC04 S09 C05 P0000250 T0000000 D0 L0 A1

ADC05 S09 C06 P0000250 T0000000 D0 L0 A1

ADC10 S10 C01 P0001000 T0000000 D0 L0 A1

ADC11 S10 C02 P0000250 T0000000 D0 L0 A1

ADC12 S10 C03 P0001000 T0000000 D0 L0 A1

ADC13 S10 C04 P0001000 T0000000 D0 L0 A1

ADC14 S10 C05 P0001000 T0000000 D0 L0 A1

DO00 S-1 C-1 E0000000 D0000000  O0 A1

BP00 S09 C07 P0000250 A1

CALIBRATION:

S09 C01 G+1.5157e-02 O+0.0000e+00

S09 C02 G+7.3240e-06 O+0.0000e+00

S09 C03 G+7.3240e-06 O+0.0000e+00

S09 C04 G+1.1100e-05 O+0.0000e+00

S09 C05 G+1.1100e-05 O+0.0000e+00

S09 C06 G+1.1100e-05 O+0.0000e+00

S10 C01 G+5.6400e-04 O+0.0000e+00

S10 C02 G+4.5780e-04 O+0.0000e+00

S10 C03 G+5.6400e-04 O+0.0000e+00

S10 C04 G+5.6400e-04 O+0.0000e+00

S10 C05 G+2.0220e-01 O-2.7315e+02

CALIBRATION REV "$Revision: 1.13 $"


</DEV_MD>
<DOC_MD>
<?xml version="1.0" encoding="UTF-8"?>
<!-- $Header: /home/cvs/puckxml/1593.xml,v 1.1 2006/10/19 23:02:01 kgomes Exp $	-->
<!-- Last edited by $Author: kgomes $	$Date: 2006/10/19 23:02:01 $   -->
<Metadata xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" 
	xsi:noNamespaceSchemaLocation="http://new-ssds.mbari.org/ssds-docs/xml/schema/SSDS_Metadata.xsd" 
	majorVersion="1" minorVersion="1" 
	lastAuthor="$Author: kgomes $" lastUpdate="$Date: 2006/10/19 23:02:01 $" >
    
	<Deployment role="instrument" >
		<Device id="1593" name="MOOS 400-12V Switch" type="Network Hub-Power Controller" mfgName="MBARI" mfgModel="MOOS 400-12V Switch" mfgSerialNumber="1.04">
			<description>MOOS Mooring BIN Power Controller</description>
			<Person firstname="Ed" surname="Mellinger" organization="MBARI" email="meed@mbari.org"/>
		</Device>
		
		<output>
			<DataStream>
				<description>Mooring Power Can data</description>
			
				<RecordDescription bufferStyle="ASCII" bufferParseType="ordered" bufferItemSeparator="whitespace" bufferLengthType="variable" parseable="true" recordType="1">
					<RecordVariable
						name="Channel ADC00 Label"
						longName="ADC00: 400V Input Volt (Channel Label)"
						units="none"
						columnIndex="1"
						format="string" >
						<description>Label for ADC00. This channel is the Channel Label for the 400V Input Voltage.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC00 Avg"
						longName="ADC00/ 400V Input Volt Avg"
						units="volts"
						columnIndex="2"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 400V Input Voltage. (Power Can channel ADC00)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC00 NumSamps"
						longName="ADC00/ 400V Input Volt Number of Samples"
						units="count"
						columnIndex="3"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Input Voltage. (Power Can channel ADC00)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC00 Min"
						longName="ADC00/ 400V Input Volt Min"
						units="volts"
						columnIndex="4"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 400V Input Voltage. (Power Can channel ADC00)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC00 Max"
						longName="ADC00/ 400V Input Volt Max"
						units="volts"
						columnIndex="5"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 400V Input Voltage. (Power Can ADC00)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC00 Err Flag"
						longName="ADC00/ 400V Input Volt Err Flag"
						units="0isgood"
						columnIndex="6"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 400V Input Voltage. (Power Can channel ADC00)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC01 Label"
						longName="ADC01: 400-12 Conv 0 In Curr (Channel Label)"
						units="none"
						columnIndex="7"
						format="string" >
						<description>Label for ADC01. This channel is the Channel Label for the 400-12 Converter 0 Input Current.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC01 Avg"
						longName="ADC01/ 400-12 Conv 0 In Curr Avg"
						units="amps"
						columnIndex="8"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 400-12 Converter 0 Input Current. (Power Can channel ADC01)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC01 NumSamps"
						longName="ADC01/ 400-12 Conv 0 In Curr Number of Samples"
						units="count"
						columnIndex="9"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400-12 Converter 0 Input Current. (Power Can channel ADC01)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC01 Min"
						longName="ADC01/ 400-12 Conv 0 In Curr Min"
						units="amps"
						columnIndex="10"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 400-12 Converter 0 Input Current. (Power Can channel ADC01)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC01 Max"
						longName="ADC01/ 400-12 Conv 0 In Curr Max"
						units="amps"
						columnIndex="11"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 400-12 Converter 0 Input Current. (Power Can ADC01)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC01 Err Flag"
						longName="ADC01/ 400-12 Conv 0 In Curr Err Flag"
						units="0isgood"
						columnIndex="12"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 400-12 Converter 0 Input Current. (Power Can channel ADC01)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC02 Label"
						longName="ADC02: 400-12 Conv 1 In Curr (Channel Label)"
						units="none"
						columnIndex="13"
						format="string" >
						<description>Label for ADC02. This channel is the Channel Label for the 400-12 Converter 1 Input Current.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC02 Avg"
						longName="ADC02/ 400-12 Conv 1 In Curr Avg"
						units="amps"
						columnIndex="14"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 400-12 Converter 1 Input Current. (Power Can channel ADC02)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC02 NumSamps"
						longName="ADC02/ 400-12 Conv 1 In Curr Number of Samples"
						units="count"
						columnIndex="15"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400-12 Converter 1 Input Current. (Power Can channel ADC02)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC02 Min"
						longName="ADC02/ 400-12 Conv 1 In Curr Min"
						units="amps"
						columnIndex="16"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 400-12 Converter 1 Input Current. (Power Can channel ADC02)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC02 Max"
						longName="ADC02/ 400-12 Conv 1 In Curr Max"
						units="amps"
						columnIndex="17"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 400-12 Converter 1 Input Current. (Power Can ADC02)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC02 Err Flag"
						longName="ADC02/ 400-12 Conv 1 In Curr Err Flag"
						units="0isgood"
						columnIndex="18"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 400-12 Converter 1 Input Current. (Power Can channel ADC02)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC03 Label"
						longName="ADC03: 400V Sw 0 Out Curr (Channel Label)"
						units="none"
						columnIndex="19"
						format="string" >
						<description>Label for ADC03. This channel is the Channel Label for the 400V Switch 0 Output Current.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC03 Avg"
						longName="ADC03/ 400V Sw 0 Out Curr Avg"
						units="amps"
						columnIndex="20"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 400V Switch 0 Output Current. (Power Can channel ADC03)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC03 NumSamps"
						longName="ADC03/ 400V Sw 0 Out Curr Number of Samples"
						units="count"
						columnIndex="21"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 0 Output Current. (Power Can channel ADC03)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC03 Min"
						longName="ADC03/ 400V Sw 0 Out Curr Min"
						units="amps"
						columnIndex="22"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 400V Switch 0 Output Current. (Power Can channel ADC03)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC03 Max"
						longName="ADC03/ 400V Sw 0 Out Curr Max"
						units="amps"
						columnIndex="23"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 400V Switch 0 Output Current. (Power Can ADC03)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC03 Err Flag"
						longName="ADC03/ 400V Sw 0 Out Curr Err Flag"
						units="0isgood"
						columnIndex="24"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 400V Switch 0 Output Current. (Power Can channel ADC03)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC04 Label"
						longName="ADC04: 400V Sw 1 Out Curr (Channel Label)"
						units="none"
						columnIndex="25"
						format="string" >
						<description>Label for ADC04. This channel is the Channel Label for the 400V Switch 1 Output Current.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC04 Avg"
						longName="ADC04/ 400V Sw 1 Out Curr Avg"
						units="amps"
						columnIndex="26"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 400V Switch 1 Output Current. (Power Can channel ADC04)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC04 NumSamps"
						longName="ADC04/ 400V Sw 1 Out Curr Number of Samples"
						units="count"
						columnIndex="27"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 1 Output Current. (Power Can channel ADC04)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC04 Min"
						longName="ADC04/ 400V Sw 1 Out Curr Min"
						units="amps"
						columnIndex="28"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 400V Switch 1 Output Current. (Power Can channel ADC04)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC04 Max"
						longName="ADC04/ 400V Sw 1 Out Curr Max"
						units="amps"
						columnIndex="29"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 400V Switch 1 Output Current. (Power Can ADC04)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC04 Err Flag"
						longName="ADC04/ 400V Sw 1 Out Curr Err Flag"
						units="0isgood"
						columnIndex="30"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 400V Switch 1 Output Current. (Power Can channel ADC04)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC05 Label"
						longName="ADC05: 400V Sw 2 Out Curr (Channel Label)"
						units="none"
						columnIndex="31"
						format="string" >
						<description>Label for ADC05. This channel is the Channel Label for the 400V Switch 2 Output Current.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC05 Avg"
						longName="ADC05/ 400V Sw 2 Out Curr Avg"
						units="amps"
						columnIndex="32"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 400V Switch 2 Output Current. (Power Can channel ADC05)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC05 NumSamps"
						longName="ADC05/ 400V Sw 2 Out Curr Number of Samples"
						units="count"
						columnIndex="33"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 2 Output Current. (Power Can channel ADC05)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC05 Min"
						longName="ADC05/ 400V Sw 2 Out Curr Min"
						units="amps"
						columnIndex="34"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 400V Switch 2 Output Current. (Power Can channel ADC05)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC05 Max"
						longName="ADC05/ 400V Sw 2 Out Curr Max"
						units="amps"
						columnIndex="35"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 400V Switch 2 Output Current. (Power Can ADC05)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC05 Err Flag"
						longName="ADC05/ 400V Sw 2 Out Curr Err Flag"
						units="0isgood"
						columnIndex="36"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 400V Switch 2 Output Current. (Power Can channel ADC05)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC10 Label"
						longName="ADC10: 12V Output Voltage (Channel Label)"
						units="none"
						columnIndex="37"
						format="string" >
						<description>Label for ADC10. This channel is the Channel Label for the 12V Output Voltage.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC10 Avg"
						longName="ADC10/ 12V Output Voltage Avg"
						units="volts"
						columnIndex="38"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 12V Output Voltage. (Power Can channel ADC10)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC10 NumSamps"
						longName="ADC10/ 12V Output Voltage Number of Samples"
						units="count"
						columnIndex="39"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 12V Output Voltage. (Power Can channel ADC10)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC10 Min"
						longName="ADC10/ 12V Output Voltage Min"
						units="volts"
						columnIndex="40"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 12V Output Voltage. (Power Can channel ADC10)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC10 Max"
						longName="ADC10/ 12V Output Voltage Max"
						units="volts"
						columnIndex="41"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 12V Output Voltage. (Power Can ADC10)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC10 Err Flag"
						longName="ADC10/ 12V Output Voltage Err Flag"
						units="0isgood"
						columnIndex="42"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 12V Output Voltage. (Power Can channel ADC10)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC11 Label"
						longName="ADC11: 12V Output Current (Channel Label)"
						units="none"
						columnIndex="43"
						format="string" >
						<description>Label for ADC11. This channel is the Channel Label for the 12V Output Current.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC11 Avg"
						longName="ADC11/ 12V Output Current Avg"
						units="amps"
						columnIndex="44"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 12V Output Current. (Power Can channel ADC11)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC11 NumSamps"
						longName="ADC11/ 12V Output Current Number of Samples"
						units="count"
						columnIndex="45"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 12V Output Current. (Power Can channel ADC11)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC11 Min"
						longName="ADC11/ 12V Output Current Min"
						units="amps"
						columnIndex="46"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 12V Output Current. (Power Can channel ADC11)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC11 Max"
						longName="ADC11/ 12V Output Current Max"
						units="amps"
						columnIndex="47"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 12V Output Current. (Power Can ADC11)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC11 Err Flag"
						longName="ADC11/ 12V Output Current Err Flag"
						units="0isgood"
						columnIndex="48"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 12V Output Current. (Power Can channel ADC11)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC12 Label"
						longName="ADC12: Ultracap Voltage (Channel Label)"
						units="none"
						columnIndex="49"
						format="string" >
						<description>Label for ADC12. This channel is the Channel Label for the Ultracap Voltage.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC12 Avg"
						longName="ADC12/ Ultracap Voltage Avg"
						units="volts"
						columnIndex="50"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for Ultracap Voltage. (Power Can channel ADC12)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC12 NumSamps"
						longName="ADC12/ Ultracap Voltage Number of Samples"
						units="count"
						columnIndex="51"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for Ultracap Voltage. (Power Can channel ADC12)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC12 Min"
						longName="ADC12/ Ultracap Voltage Min"
						units="volts"
						columnIndex="52"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for Ultracap Voltage. (Power Can channel ADC12)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC12 Max"
						longName="ADC12/ Ultracap Voltage Max"
						units="volts"
						columnIndex="53"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for Ultracap Voltage. (Power Can ADC12)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC12 Err Flag"
						longName="ADC12/ Ultracap Voltage Err Flag"
						units="0isgood"
						columnIndex="54"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for Ultracap Voltage. (Power Can channel ADC12)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC13 Label"
						longName="ADC13: Batt Voltage (Channel Label)"
						units="none"
						columnIndex="55"
						format="string" >
						<description>Label for ADC13. This channel is the Channel Label for the Battery Voltage.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC13 Avg"
						longName="ADC13/ Batt Voltage Avg"
						units="volts"
						columnIndex="56"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for Battery Voltage. (Power Can channel ADC13)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC13 NumSamps"
						longName="ADC13/ Batt Voltage Number of Samples"
						units="count"
						columnIndex="57"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for Battery Voltage. (Power Can channel ADC13)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC13 Min"
						longName="ADC13/ Batt Voltage Min"
						units="volts"
						columnIndex="58"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for Battery Voltage. (Power Can channel ADC13)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC13 Max"
						longName="ADC13/ Batt Voltage Max"
						units="volts"
						columnIndex="59"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for Battery Voltage. (Power Can ADC13)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC13 Err Flag"
						longName="ADC13/ Batt Voltage Err Flag"
						units="0isgood"
						columnIndex="60"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for Battery Voltage. (Power Can channel ADC13)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel ADC14 Label"
						longName="ADC14: 400-12 Converter Temp (Channel Label)"
						units="none"
						columnIndex="61"
						format="string" >
						<description>Label for ADC14. This channel is the Channel Label for the 400-12 Converter Temperature.</description>
					</RecordVariable>
					<RecordVariable
						name="ADC14 Avg"
						longName="ADC14/ 400-12 Converter Temp Avg"
						units="deg C"
						columnIndex="62"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Average for 400-12 Converter Temperature. (Power Can channel ADC14)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC14 NumSamps"
						longName="ADC14/ 400-12 Converter Temp Number of Samples"
						units="count"
						columnIndex="63"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400-12 Converter Temperature. (Power Can channel ADC14)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC14 Min"
						longName="ADC14/ 400-12 Converter Temp Min"
						units="deg C"
						columnIndex="64"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Minimum for 400-12 Converter Temperature. (Power Can channel ADC14)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC14 Max"
						longName="ADC14/ 400-12 Converter Temp Max"
						units="deg C"
						columnIndex="65"
						format="double" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Maximum for 400-12 Converter Temperature. (Power Can ADC14)</description>
					</RecordVariable>
					<RecordVariable
						name="ADC14 Err Flag"
						longName="ADC14/ 400-12 Converter Temp Err Flag"
						units="0isgood"
						columnIndex="66"
						format="int" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Error Flag Value for 400-12 Converter Temperature. (Power Can channel ADC14)</description>
					</RecordVariable>

					<RecordVariable
						name="Channel BP00 Label"
						longName="BP00: 400V Status (Channel Label)"
						units="none"
						columnIndex="67"
						format="string" >
						<description>Label for BP00. This channel is the Channel Label for the 400V Status Bits.</description>
					</RecordVariable>
					<RecordVariable
						name="BP00 NumSamps"
						longName="BP00/ 400V Status Number of Samples"
						units="count"
						columnIndex="68"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Status Bits. (Power Can channel BP00)</description>
					</RecordVariable>

					<RecordVariable
						name="BP00-0 NumSamps"
						longName="BP00-0/  Number of Samples"
						units="count"
						columnIndex="69"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400-12 Converter 0 CB OK Flag. (Power Can channel BP00-0)</description>
					</RecordVariable>

					<RecordVariable
						name="BP00-1 NumSamps"
						longName="BP00-1/  Number of Samples"
						units="count"
						columnIndex="70"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400-12 Converter 1 CB OK Flag. (Power Can channel BP00-1)</description>
					</RecordVariable>

					<RecordVariable
						name="BP00-2 NumSamps"
						longName="BP00-2/  Number of Samples"
						units="count"
						columnIndex="71"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 0 On Flag. (Power Can channel BP00-2)</description>
					</RecordVariable>

					<RecordVariable
						name="BP00-3 NumSamps"
						longName="BP00-3/  Number of Samples"
						units="count"
						columnIndex="72"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 0 CB OK Flag. (Power Can channel BP00-3)</description>
					</RecordVariable>

					<RecordVariable
						name="BP00-4 NumSamps"
						longName="BP00-4/  Number of Samples"
						units="count"
						columnIndex="73"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 1 On Flag. (Power Can channel BP00-4)</description>
					</RecordVariable>

					<RecordVariable
						name="BP00-5 NumSamps"
						longName="BP00-5/  Number of Samples"
						units="count"
						columnIndex="74"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 1 CB OK Flag. (Power Can channel BP00-5)</description>
					</RecordVariable>

					<RecordVariable
						name="BP00-6 NumSamps"
						longName="BP00-6/  Number of Samples"
						units="count"
						columnIndex="75"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 2 On Flag. (Power Can channel BP00-6)</description>
					</RecordVariable>

					<RecordVariable
						name="BP00-7 NumSamps"
						longName="BP00-7/  Number of Samples"
						units="count"
						columnIndex="76"
						format="long" parseRegExp="^[A-Z]+([-+0-9].*)" >
							<description>The Number of Samples for 400V Switch 2 CB OK Flag. (Power Can channel BP00-7)</description>
					</RecordVariable>
					<RecordVariable
					     name="CheckString Data" 
					     longName="CheckString Data" 
					     units="string" 
					     columnIndex="77" format="string">
						<description>Just the word DATA</description>
					</RecordVariable>
					<RecordVariable 
					     name="CheckString Count"
					     longName="CheckString Count" 
					     units="string"
					     columnIndex="78" format="string">
						<description>Just the word COUNT</description>
					</RecordVariable>
					<RecordVariable 
					     name="Data Count"
					     longName="Number of bytes transmitted in record" 
					     units="count" columnIndex="79" format="int">
						<description>Total bytes transmitted</description>
					</RecordVariable>
				</RecordDescription>
			</DataStream>
		</output>
	</Deployment>
</Metadata>

</DOC_MD>

Press any key to show schedule for instrument on  /dev/ttySX13 :3 [main] DEBUG moos.operations.utils.NodeUtility  - getNodeURL(): input=//loc/node
104 [main] ERROR moos.operations.utils.ShowSchedule  - ShowSchedule: lookAhead value undefined or invalid; using default (3600)
105 [main] DEBUG moos.operations.utils.ShowSchedule  - Looking for node service at rmi://loc/node
865 [main] DEBUG moos.utils.SiamSocketFactory  - SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
866 [main] DEBUG moos.utils.SiamSocketFactory  - return new Socket(host, port)...
1807 [main] DEBUG moos.utils.SiamSocketFactory  - SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1808 [main] DEBUG moos.utils.SiamSocketFactory  - return new Socket(host, port)...
2026 [main] DEBUG moos.operations.utils.ShowSchedule  - Got proxy for node service "moos.deployed.NodeService"

 
    Name: Default
   Owner: moos.devices.serialadc.PowerCan:1593 key=7
Schedule: R */0 */10 */0 */0 * * * * GMT *
  Status: Waiting	546189


1 DEBUG  NodeUtility [main]: getNodeURL(): input=//loc/node
Looking for node server stub at rmi://loc/node
610 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=loc, port=1099, server host=loc
611 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
1976 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
1977 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Got proxy for node service "moos.deployed.NodeService"
2978 DEBUG  SiamSocketFactory [main]: SiamSocketFactory.createSocket() - host=134.89.36.11, port=1025, server host=loc
2980 DEBUG  SiamSocketFactory [main]: return new Socket(host, port)...
Test complete.



