ASIMET WND (ID 1291)
1. Commands issued to instrument by service at initialization 

None
2. Commands issued by service for safe mode, if applicable
N/A
3. Device metadata returned in SIAM datastream
4. Instrument-specific service properties
               String sensorType = WND;

       String moduleAddress = 01;
5. Initial service property values for this deployment
moduleAddress=01 
sensorType=WND
powerOnDelaySec=0 
nominalCurrentMa=1000 
serviceName=ASIMET WND s/n WND358 
maxSummarySamples=0 
currentLimitMa=3000 
packetSetSize=10 
sampleSchedule=R */0 */10 */0 */0 * * * * GMT * defaultSkipInterval=0 
extendedVersion=UNK 
frameworkVersion=$Name: june09_2006 $ 
UUID=E1C9B97E-DF52-4F54-BB92-C8B1C6551003 powerPolicy=SAMPLING 
isiID=1291 
peakCurrentMa=5000 
summaryTriggerCount=0 
sampleTimeoutMsec=3000 
commPowerPolicy=SAMPLING 
startDelayMsec=4000 (modify to 60000) 
6. Results of acceptance test procedures
7. Summarization

8. Instrument clock synchronization

8. Known-service bugs/deficiencies







