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Solar/Battery Interface Board





Schematic and BOM # 1002300


PWB #1002333 "SOLARBATTBOARD"





1.	Install CI5/CI6 "DIN Power Contact" in six places provided on connector P5, "DIN_42+6". 





2.	Do not install R7, R8, R9, R10 (values TBD at MBARI)





3.	Do not install JMP1, JMP2.





4.	This board uses 2 oz copper.   Please adjust solder profiles accordingly.





