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ISUS has two user interface modes, an interactive Menu Mode and a more terse Command Mode, one of the commands being the M command, for entering Menu Mode. The remaining commands in the Command Mode set are as follows:

ISUS COMMANDS (W,E,T,R,D):

W

Desc: Query ISUS for heartbeat.



Output: ACK



Output Type: string

E

Desc: Query ISUS for its current RTC value.



Output: Epoch (Jan 01, 1970) seconds.



Output Type: unsigned long int (ulong).

T,val

Desc: Set ISUS's RTC(s).



Argument: val, Epoch (Jan 01, 1970) seconds.



Argument Type: 
chars (up to 20) read one at a





time (until CR/LF) and converted





to ulong.




Output: ACK,value sent, value set and read back.



Output Type: string,ulong,ulong





Error Output(s):

               
NACK,GetCharTimeout!
pace timeout is 3 secs max.

               
NACK,GetCharOverflow!

20 char max.

                  
NACK,NoDataSeperator!

no comma found.

                  
NACK,ULongIntInvalid!

conversion failure.

                  
NACK,ULongIntOverflow! 
conversion overflow.

R

Desc: Query ISUS for # of pending data records.



Output: ASCII formatted number



Output Type: unsigned long int (ulong).

D

Desc: Request data from FIFO spool file



Output: ISUS Data Record (scans)

