0 0.2 0.4 0.6 0.8 1 1.2 1.4 1.6 1.8 2 -2

-1.8

-1.6

-1.4

-1.2

-1

-0.8

-0.6

-0.4

-0.2

0

time (seconds after anchor impact) meters

Landing Transient of Termination after Anchor Touchdown Inertial Considerations only, Drag neglected m = 1000 kg, 1.8 m X 1.5 m cylinder

Vel = -1 m/s Vel = -2 m/s Vel = -3 m/s