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Description:

· Cyclic bending test of cable clamp.  Specimen has fish-bite which ends at cable clamp.  Clamp is loaded with 500lbs weight to simulate axial loads due to floats.
· +/- 50 degrees, 200-5300lbs

· 235,000 bend cycles, cable rotated 90 degrees after 115,000 cycles.

Results:

· Sample cut 117” from center of the pin in the Crosby socket before breaking.

