/**
 * \defgroup uipopt Configuration options for uIP
 * @{
 *
 * uIP is configured using the per-project configuration file
 * "uipopt.h". This file contains all compile-time options for uIP and
 * should be tweaked to match each specific project. The uIP
 * distribution contains a documented example "uipopt.h" that can be
 * copied and modified for each project.
 */

/**
 * \file
 * Configuration options for uIP.
 * \author Adam Dunkels <adam@dunkels.com>
 *
 * This file is used for tweaking various configuration options for
 * uIP. You should make a copy of this file into one of your project's
 * directories instead of editing this example "uipopt.h" file that
 * comes with the uIP distribution.
 */

/*
 * Copyright (c) 2001-2003, Adam Dunkels.
 * All rights reserved. 
 *
 * Redistribution and use in source and binary forms, with or without 
 * modification, are permitted provided that the following conditions 
 * are met: 
 * 1. Redistributions of source code must retain the above copyright 
 *    notice, this list of conditions and the following disclaimer. 
 * 2. Redistributions in binary form must reproduce the above copyright 
 *    notice, this list of conditions and the following disclaimer in the 
 *    documentation and/or other materials provided with the distribution. 
 * 3. The name of the author may not be used to endorse or promote
 *    products derived from this software without specific prior
 *    written permission.  
 *
 * THIS SOFTWARE IS PROVIDED BY THE AUTHOR ``AS IS'' AND ANY EXPRESS
 * OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
 * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
 * ARE DISCLAIMED.  IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
 * DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
 * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE
 * GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
 * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY,
 * WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
 * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
 * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.  
 *
 * This file is part of the uIP TCP/IP stack.
 *
 * $Id: uipopt.h,v 1.16.2.5 2003/10/07 13:22:51 adam Exp $
 *
 */

#ifndef __UIPOPT_H__
#define __UIPOPT_H__

/*------------------------------------------------------------------------------*/
/**
 * \defgroup uipopttypedef uIP type definitions
 * @{
 */

/**
 * The 8-bit unsigned data type.
 *
 * This may have to be tweaked for your particular compiler. "unsigned
 * char" works for most compilers.
 */
typedef unsigned char u8_t;

/**
 * The 16-bit unsigned data type.
 *
 * This may have to be tweaked for your particular compiler. "unsigned
 * short" works for most compilers.
 */
typedef unsigned short u16_t;

/**
 * The statistics data type.
 *
 * This datatype determines how high the statistics counters are able
 * to count.
 */
typedef unsigned short uip_stats_t;

/** @} */

/*------------------------------------------------------------------------------*/

/**
 * \defgroup uipoptstaticconf Static configuration options
 * @{
 *
 * These configuration options can be used for setting the IP address
 * settings statically, but only if UIP_FIXEDADDR is set to 1. The
 * configuration options for a specific node includes IP address,
 * netmask and default router as well as the Ethernet address. The
 * netmask, default router and Ethernet address are appliciable only
 * if uIP should be run over Ethernet.
 *
 * All of these should be changed to suit your project.
*/

/**
 * Determines if uIP should use a fixed IP address or not.
 *
 * If uIP should use a fixed IP address, the settings are set in the
 * uipopt.h file. If not, the macros uip_sethostaddr(),
 * uip_setdraddr() and uip_setnetmask() should be used instead.
 *
 * \hideinitializer
 */
#define UIP_FIXEDADDR    1

/**
 * Ping IP address asignment.
 *
 * uIP uses a "ping" packets for setting its own IP address if this
 * option is set. If so, uIP will start with an empty IP address and
 * the destination IP address of the first incoming "ping" (ICMP echo)
 * packet will be used for setting the hosts IP address.
 *
 * \note This works only if UIP_FIXEDADDR is 0.
 *
 * \hideinitializer
 */
#define UIP_PINGADDRCONF 0

#if 0
#define UIP_IPADDR0     192U /**< The first octet of the IP address of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_IPADDR1     168U /**< The second octet of the IP address of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_IPADDR2     0U   /**< The third octet of the IP address of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_IPADDR3     30U  /**< The fourth octet of the IP address of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */

#define UIP_NETMASK0    255 /**< The first octet of the netmask of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_NETMASK1    255 /**< The second octet of the netmask of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_NETMASK2    255 /**< The third octet of the netmask of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_NETMASK3    0   /**< The fourth octet of the netmask of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */


#define UIP_DRIPADDR0   192 /**< The first octet of the IP address of
			       the default router, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_DRIPADDR1   168 /**< The second octet of the IP address of
			       the default router, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_DRIPADDR2   0   /**< The third octet of the IP address of
			       the default router, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_DRIPADDR3   1   /**< The fourth octet of the IP address of
			       the default router, if UIP_FIXEDADDR is
			       1. \hideinitializer */

#else

#define UIP_IPADDR0     10U  /**< The first octet of the IP address of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_IPADDR1     0U /**< The second octet of the IP address of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_IPADDR2     0U   /**< The third octet of the IP address of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_IPADDR3     30U  /**< The fourth octet of the IP address of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */

#define UIP_NETMASK0    255 /**< The first octet of the netmask of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_NETMASK1    255 /**< The second octet of the netmask of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_NETMASK2    255 /**< The third octet of the netmask of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_NETMASK3    0   /**< The fourth octet of the netmask of
			       this uIP node, if UIP_FIXEDADDR is
			       1. \hideinitializer */

#define UIP_DRIPADDR0   10 /**< The first octet of the IP address of
			       the default router, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_DRIPADDR1   0 /**< The second octet of the IP address of
			       the default router, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_DRIPADDR2   0   /**< The third octet of the IP address of
			       the default router, if UIP_FIXEDADDR is
			       1. \hideinitializer */
#define UIP_DRIPADDR3   1   /**< The fourth octet of the IP address of
			       the default router, if UIP_FIXEDADDR is
			       1. \hideinitializer */

#endif

/**
 * Specifies if the uIP ARP module should be compiled with a fixed
 * Ethernet MAC address or not.
 *
 * If this configuration option is 0, the macro uip_setethaddr() can
 * be used to specify the Ethernet address at run-time.
 *
 * \hideinitializer
 */
#define UIP_FIXEDETHADDR 0

#define UIP_ETHADDR0    0x00  /**< The first octet of the Ethernet
				 address if UIP_FIXEDETHADDR is
				 1. \hideinitializer */
#define UIP_ETHADDR1    0xbd  /**< The second octet of the Ethernet
				 address if UIP_FIXEDETHADDR is
				 1. \hideinitializer */
#define UIP_ETHADDR2    0x3b  /**< The third octet of the Ethernet
				 address if UIP_FIXEDETHADDR is
				 1. \hideinitializer */
#define UIP_ETHADDR3    0x33  /**< The fourth octet of the Ethernet
				 address if UIP_FIXEDETHADDR is
				 1. \hideinitializer */
#define UIP_ETHADDR4    0x05  /**< The fifth octet of the Ethernet
				 address if UIP_FIXEDETHADDR is
				 1. \hideinitializer */
#define UIP_ETHADDR5    0x71  /**< The sixth octet of the Ethernet
				 address if UIP_FIXEDETHADDR is
				 1. \hideinitializer */

/** @} */
/*------------------------------------------------------------------------------*/
/**
 * \defgroup uipoptip IP configuration options
 * @{
 *
 */
/**
 * The IP TTL (time to live) of IP packets sent by uIP.
 *
 * This should normally not be changed.
 */
#define UIP_TTL         255

/**
 * Turn on support for IP packet reassembly.
 *
 * uIP supports reassembly of fragmented IP packets. This features
 * requires an additonal amount of RAM to hold the reassembly buffer
 * and the reassembly code size is approximately 700 bytes.  The
 * reassembly buffer is of the same size as the uip_buf buffer
 * (configured by UIP_BUFSIZE).
 *
 * \note IP packet reassembly is not heavily tested.
 *
 * \hideinitializer
 */
#define UIP_REASSEMBLY 0

/**
 * The maximum time an IP fragment should wait in the reassembly
 * buffer before it is dropped.
 *
 */
#define UIP_REASS_MAXAGE 40

/** @} */

/*------------------------------------------------------------------------------*/
/**
 * \defgroup uipoptudp UDP configuration options
 * @{
 *
 * \note The UDP support in uIP is still not entirely complete; there
 * is no support for sending or receiving broadcast or multicast
 * packets, but it works well enough to support a number of vital
 * applications such as DNS queries, though
 */

/**
 * Toggles wether UDP support should be compiled in or not.
 *
 * \hideinitializer
 */
#define UIP_UDP           0

/**
 * Toggles if UDP checksums should be used or not.
 *
 * \note Support for UDP checksums is currently not included in uIP,
 * so this option has no function.
 *
 * \hideinitializer
 */
#define UIP_UDP_CHECKSUMS 0

/**
 * The maximum amount of concurrent UDP connections.
 *
 * \hideinitializer
 */
#define UIP_UDP_CONNS    2

/**
 * The name of the function that should be called when UDP datagrams arrive.
 *
 * \hideinitializer
 */
#define UIP_UDP_APPCALL  udp_appcall

/** @} */
/*------------------------------------------------------------------------------*/
/**
 * \defgroup uipopttcp TCP configuration options
 * @{
 */

/**
 * Determines if support for opening connections from uIP should be
 * compiled in.
 *
 * If the applications that are running on top of uIP for this project
 * do not need to open outgoing TCP connections, this configration
 * option can be turned off to reduce the code size of uIP.
 *
 * \hideinitializer
 */
#define UIP_ACTIVE_OPEN 1

/**
 * The maximum number of simultaneously open TCP connections.
 *
 * Since the TCP connections are statically allocated, turning this
 * configuration knob down results in less RAM used. Each TCP
 * connection requires approximatly 30 bytes of memory.
 *
 * \hideinitializer
 */
#define UIP_CONNS       10

/**
 * The maximum number of simultaneously listening TCP ports.
 *
 * Each listening TCP port requires 2 bytes of memory.
 *
 * \hideinitializer
 */
#define UIP_LISTENPORTS 10

/**
 * The size of the advertised receiver's window.
 *
 * Should be set low (i.e., to the size of the uip_buf buffer) is the
 * application is slow to process incoming data, or high (32768 bytes)
 * if the application processes data quickly.
 *
 * \hideinitializer
 */
#define UIP_RECEIVE_WINDOW   32768

/**
 * Determines if support for TCP urgent data notification should be
 * compiled in.
 *
 * Urgent data (out-of-band data) is a rarely used TCP feature that
 * very seldom would be required.
 *
 * \hideinitializer
 */
#define UIP_URGDATA      1

/**
 * The initial retransmission timeout counted in timer pulses.
 *
 * This should not be changed.
 */
#define UIP_RTO         3

/**
 * The maximum number of times a segment should be retransmitted
 * before the connection should be aborted.
 *
 * This should not be changed.
 */
#define UIP_MAXRTX      8

/**
 * The maximum number of times a SYN segment should be retransmitted
 * before a connection request should be deemed to have been
 * unsuccessful.
 *
 * This should not need to be changed.
 */
#define UIP_MAXSYNRTX      3

/**
 * The TCP maximum segment size.
 *
 * This is should not be to set to more than UIP_BUFSIZE - UIP_LLH_LEN - 40.
 */
#define UIP_TCP_MSS     (UIP_BUFSIZE - UIP_LLH_LEN - 40)

/**
 * How long a connection should stay in the TIME_WAIT state.
 *
 * This configiration option has no real implication, and it should be
 * left untouched.
 */ 
#define UIP_TIME_WAIT_TIMEOUT 120


/** @} */
/*------------------------------------------------------------------------------*/
/**
 * \defgroup uipoptarp ARP configuration options
 * @{
 */

/**
 * The size of the ARP table.
 *
 * This option should be set to a larger value if this uIP node will
 * have many connections from the local network.
 *
 * \hideinitializer
 */
#define UIP_ARPTAB_SIZE 8

/**
 * The maxium age of ARP table entries measured in 10ths of seconds.
 *
 * An UIP_ARP_MAXAGE of 120 corresponds to 20 minutes (BSD
 * default).
 */
#define UIP_ARP_MAXAGE 120

/** @} */

/*------------------------------------------------------------------------------*/

/**
 * \defgroup uipoptgeneral General configuration options
 * @{
 */

/**
 * The size of the uIP packet buffer.
 *
 * The uIP packet buffer should not be smaller than 60 bytes, and does
 * not need to be larger than 1500 bytes. Lower size results in lower
 * TCP throughput, larger size results in higher TCP throughput.
 *
 * \hideinitializer
 */
#define UIP_BUFSIZE     1800


/**
 * Determines if statistics support should be compiled in.
 *
 * The statistics is useful for debugging and to show the user.
 *
 * \hideinitializer
 */
#define UIP_STATISTICS  1

/**
 * Determines if logging of certain events should be compiled in.
 *
 * This is useful mostly for debugging. The function uip_log()
 * must be implemented to suit the architecture of the project, if
 * logging is turned on.
 *
 * \hideinitializer
 */
#define UIP_LOGGING 0

/**
 * Print out a uIP log message.
 *
 * This function must be implemented by the module that uses uIP, and
 * is called by uIP whenever a log message is generated.
 */
void uip_log(char *msg);

/**
 * The link level header length.
 *
 * This is the offset into the uip_buf where the IP header can be
 * found. For Ethernet, this should be set to 14. For SLIP, this
 * should be set to 0.
 *
 * \hideinitializer
 */
#define UIP_LLH_LEN     14


/** @} */
/*------------------------------------------------------------------------------*/
/**
 * \defgroup uipoptcpu CPU architecture configuration
 * @{
 *
 * The CPU architecture configuration is where the endianess of the
 * CPU on which uIP is to be run is specified. Most CPUs today are
 * little endian, and the most notable exception are the Motorolas
 * which are big endian. The BYTE_ORDER macro should be changed to
 * reflect the CPU architecture on which uIP is to be run.
 */
#ifndef LITTLE_ENDIAN
#define LITTLE_ENDIAN  3412
#endif /* LITTLE_ENDIAN */
#ifndef BIG_ENDIAN
#define BIG_ENDIAN     1234
#endif /* BIGE_ENDIAN */

/**
 * The byte order of the CPU architecture on which uIP is to be run.
 *
 * This option can be either BIG_ENDIAN (Motorola byte order) or
 * LITTLE_ENDIAN (Intel byte order).
 *
 * \hideinitializer
 */
#ifndef BYTE_ORDER
#define BYTE_ORDER     LITTLE_ENDIAN
#endif /* BYTE_ORDER */

/** @} */
/*------------------------------------------------------------------------------*/

/**
 * \defgroup uipoptapp Appication specific configurations
 * @{
 *
 * An uIP application is implemented using a single application
 * function that is called by uIP whenever a TCP/IP event occurs. The
 * name of this function must be registered with uIP at compile time
 * using the UIP_APPCALL definition.
 *
 * uIP applications can store the application state within the
 * uip_conn structure by specifying the size of the application
 * structure with the UIP_APPSTATE_SIZE macro.
 *
 * The file containing the definitions must be included in the
 * uipopt.h file.
 *
 * The following example illustrates how this can look.
 \code

void httpd_appcall(void);
#define UIP_APPCALL     httpd_appcall

struct httpd_state {
  u8_t state; 
  u16_t count;
  char *dataptr;
  char *script;
};
#define UIP_APPSTATE_SIZE (sizeof(struct httpd_state))
 \endcode
 */

/**
 * \var #define UIP_APPCALL
 *
 * The name of the application function that uIP should call in
 * response to TCP/IP events.
 *
 */

/**
 * \var #define UIP_APPSTATE_SIZE
 *
 * The size of the application state that is to be stored in the
 * uip_conn structure.
 */
/** @} */

/* Include the header file for the application program that should be
   used. If you don't use the example web server, you should change
   this. */
#include "httpd.h"


#endif /* __UIPOPT_H__ */
