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1.0 INTRODUCTION.

The Monterey Aquarium Research Institute MBARI is developing a deep ocean underwater science observatory. The maximum working depth of the observatory is planned to be 4000 meters. The observatory design includes a wave following buoy system connected to a seafloor anchor with an electro-optical cable strength member referred to as the Riser Cable. 

An initial test mooring is going to be placed in Monterey Bay in Fall, 2001. This test mooring will be placed in a depth of 1800 meters. To prevent damage to the riser cable due to fish bite, the cable shall be armored along the entire length for this mooring. The initial purchase shall be for this riser cable. The total length, including scope, should be approximately 2400 meters. Since the riser will not include a swivel, it is important that the cable be torque balance as much as possible. 
It is MBARI’s intention that the cable vendor, not MBARI or its independent contractors, design the cable described in this document. Section 2.0, Performance Requirements, represents MBARI’s only firm requirements.    Items indicated as To Be Determined (TBD) are open to further discussion between MBARI and the vendor.

2.0 PERFORMANCE REQUIREMENTS.

2.1 General and Environmental. The riser cable performance shall not be degraded by conditions typical of the working environment, including:

2.1.1 Continuous submergence in seawater over working life.

2.1.2 Temperatures from 0 to 25 degrees Centigrade. 

2.1.3 Hydrostatic pressure equivalent to 4000 meters seawater (vendor should advise on cable suitability for 6000 meter operation).

2.1.4 Materials Compatibility TBD

2.1.5 Storage Conditions. TBD

2.1.6 Service Life.  The Riser cable shall provide a minimum of three years of service while continuously submerged in a dynamic ocean environment.


2.2 Mechanical
2.2.1 Diameter (minimize)

2.2.2 Weights (minimize)

2.2.3 Working Strength 6000

2.2.4 Breaking Strength 18000

2.2.5 Fatigue Life TBD

2.2.6 Elongation TBD

2.2.7 Rotation TBD

2.2.8 Minimum Bend Radius 18” or less

2.2.9 Packaging TBD


2.3 Optical


2.3.1 Fiber Count. There shall nominally be four single-mode optical fibers. In the interests of minimizing overall cable diameter, depending on cable construction and efficiencies of fiber packaging, the cabled fiber count can be reduced to an absolute minimum of three optical fibers. Fibers shall be Corning “Titan SMF CPC5” or other suitable fiber selected by cable vendor. Use of alternate fiber shall be by written agreement between vendor and MBARI. The optical specifications must be met over the specified cable service life during continuous operation under the conditions described in the “General and Environmental” and the “Mechanical” sections above.

2.3.2 Optical Attenuation. Attenuation in each fiber shall not exceed the following values under cable working conditions (see mechanical specifications for working condition values):

0.7 dB per kilometer at 1310 Nm. wavelength

0.7 dB per kilometer at 1550 Nm. wavelength

2.3.3 Optical Attenuation Uniformity. No single point attenuation discontinuity in any fiber in the finished cable shall be greater than 0.15 dB at either 1310 Nm. or 1550nm. wavelengths, as measured with an OTDR.

2.3.4 Optical Dispersion. Individual fiber specifications for optical dispersion in the completed cable shall meet the pre-cabled fiber manufacturer’s specifications for the fiber used, as measured by EIA/TIA 455-175.

2.3.5 Fiber Proof Test. Individual fibers will be proof tested at the time of manufacture to a minimum of 150kpsi.

2.3.6 Fiber Identification.  Fibers or their over-jacketing shall be color coded or otherwise indelibly marked at least every meter for identification.  


2.4  Electrical


2.4.1 General.  The cable will be used for electrical power transmission while submerged in the marine environment.  The cable shall provide a minimum of two electrical conductors insulated from one another, and from seawater.


2.4.2 Working Voltage.  The cable will be used at a working voltage between conductors, or between conductors and seawater, of up to 425 Volts DC.   At this voltage, the maximum electrical stress present at any point in the cable insulation system shall be less than or equal to 2.0 kV/mm (51 volts/mil).  The insulation system used must be suitable for continuous high D.C. electric field stress.


2.4.3 Insulation Resistance.  The Insulation Resistance of each conductor in the as-built cable shall be a minimum of 3,000 Megohms per kilometer, measured at the working voltage of Section 1.4.2 above.  The resistance shall be measured between the test conductor, and the other conductor(s) plus the cable armor plus any other metallic cable elements, tied together.


2.4.4 Conductor Resistance.  The cable will be used at a working current of up to one ampere per conductor.  The maximum as-built, as-cabled, round trip (two way) resistance of the two cable conductors in series shall be a maximum of 8.6 ohms per kilometer (nominally 4.3 ohms per kilometer per conductor, although equal resistances are not required), measured at a conductor temperature of 20 degrees C.  The as-built conductor resistance shall have a tolerance of +/- 5%.


2.4.5 Production Testing.   Each individually insulated conductor shall be tested for insulation resistance, before cable assembly, in a water bath.  The test conditions and criteria for acceptance shall be as specified in Section 1.4.3 above.  The completed cable shall be evaluated for Partial Discharge at the working voltage of Section 1.4.2 above.  No detectable discharge is permitted, within the detection limits of the test equipment employed.


2.4.6 Conductor Identification.   The individual conductors shall be color coded or otherwise made visually distinguishable from one another, either throughout their length, or at regular increments not to exceed 0.33 meter. 


3.0 QUALIFICATION TESTS. 

The following tests will be performed by MBARI or an independent test contractor at MBARI expense prior to final acceptance of the completed cable.


3.1 Electrical. A riser cable specimen will be subjected to conductor resistance and insulation resistance tests to obtain the as delivered values.
3.2 Optical Static Attenuation. The riser cable will be tested for optical attenuation at 1310Nm and 1550Nm wavelengths to obtain the as delivered values.
3.3 Optical Characterization. The optical attenuation in response to tensile loading will be measured.
3.4 Mechanical Characterization. A riser cable section will be tested for tension induced changes in elongation, diameter, torque and rotation. The riser cable will also be tested for yield and breaking strength. 
4.0 DELIVERY.

Delivery shall be quoted FOB Moss Landing, California, 95039.

Cable shall be delivered suitably packaged for transportation and storage.

Cable shall be delivered in a continuous length of 2400 meters. A minimum of five meters shall be accessible at both ends of the cable to allow testing on the shipping drum.

